[index] CentreCOM 8948XL コマンドリファレンス 2.9

# SET IP AUTONOMOUS

カテゴリー：IP / 経路制御（BGP-4）
備考：フィーチャーライセンス AT-FL-09 が必要

`SET IP AUTONOMOUS=1..65534`

自AS（Autonomous System）番号を設定する。

パラメーター

AUTONOMOUS: AS番号

備考・注意事項

自AS番号はSHOW IPコマンドで確認できる（「Autonomous System Number」欄）。
ASコンフェデレーションを構成するときは、自AS番号としてサブAS番号を設定する。コンフェデレーションAS番号はSET BGPコマンドのCONFEDERATIONIDパラメーターで指定する。

関連コマンド

ADD BGP PEER
DELETE BGP PEER
DISABLE BGP PEER
ENABLE BGP PEER
SHOW BGP PEER
SHOW IP

参考

RFC1771, A Border Gateway Protocol 4 (BGP-4)
RFC1772, Application of the Border Gateway Protocol in the Internet
RFC1930, Guidelines for creation, selection, and registration of an Autonomous System (AS)
RFC1997, BGP Communities Attribute
RFC2385, Protection of BGP Sessions via the TCP MD5 Signature Option
RFC2439, BGP Route Flap Damping
RFC2796, BGP Route Reflection - An Alternative to Full Mesh IBGP
RFC2842, Capabilities Advertisement with BGP-4
RFC2918, Route Refresh Capability for BGP-4
RFC3065, Autonomous System Confederations for BGP

(C) 2004 - 2008 アライドテレシスホールディングス株式会社

PN: J613-M0021-12 Rev.L