[index] CentreCOM 8948XL コマンドリファレンス 2.9

# RESET BGP PEER

カテゴリー：IP / 経路制御（BGP-4）
備考：フィーチャーライセンス AT-FL-09 が必要

`RESET BGP PEER={ALL|ipadd} [SOFT={IN|OUT|ALL}]`

ipadd: IPアドレス

指定したピアとのBGPセッションをリセットする。
SOFTパラメーターを指定しなかった場合は、指定したピアとのセッションをいったん切断し、その後再接続して経路情報を更新する。
SOFTパラメーターを指定した場合は、指定したピアとのBGPセッションをリセットすることなく、経路情報だけを更新する（ソフトリセット）。

パラメーター

PEER: BGPピアのIPアドレス

SOFT: 経路を更新する方向。ソフトリセット時に指定する。INを指定した場合は、該当ピアにROUTE-REFRESHメッセージを送信して、経路情報の再送信を要求する。OUTを指定した場合は、単に該当ピアに経路情報を送信しなおす。ALLを指定した場合は、INとOUTの両方の動作を行う。

関連コマンド

DISABLE BGP PEER
ENABLE BGP AUTOSOFTUPDATE
ENABLE BGP PEER
SET BGP PEER
SHOW BGP PEER

参考

RFC1771, A Border Gateway Protocol 4 (BGP-4)
RFC1772, Application of the Border Gateway Protocol in the Internet
RFC1930, Guidelines for creation, selection, and registration of an Autonomous System (AS)
RFC1997, BGP Communities Attribute
RFC2385, Protection of BGP Sessions via the TCP MD5 Signature Option
RFC2439, BGP Route Flap Damping
RFC2796, BGP Route Reflection - An Alternative to Full Mesh IBGP
RFC2842, Capabilities Advertisement with BGP-4
RFC2918, Route Refresh Capability for BGP-4
RFC3065, Autonomous System Confederations for BGP

(C) 2004 - 2008 アライドテレシスホールディングス株式会社

PN: J613-M0021-12 Rev.L