[index] CentreCOM 8948XL コマンドリファレンス 2.9

# SHOW BGP IMPORT

カテゴリー：IP / 経路制御（BGP-4）
備考：フィーチャーライセンス AT-FL-09 が必要

`SHOW BGP IMPORT`

BGPへの経路取り込み設定を表示する。

入力・出力・画面例

    Manager > show bgp import

    BGP import entries

    Proto      Route map
    --------------------------
    STATIC     -
    --------------------------

表 1
Proto | 経路情報のソース（起源）。RIP、OSPF、STATIC（静的経路）、INTERFACE（インターフェース経路）がある
Route map | インポート時に適用するルートマップ名

関連コマンド

ADD BGP IMPORT
ADD IP ROUTEMAP
DELETE BGP IMPORT
SET BGP IMPORT

参考

RFC1771, A Border Gateway Protocol 4 (BGP-4)
RFC1772, Application of the Border Gateway Protocol in the Internet
RFC1930, Guidelines for creation, selection, and registration of an Autonomous System (AS)
RFC1997, BGP Communities Attribute
RFC2385, Protection of BGP Sessions via the TCP MD5 Signature Option
RFC2439, BGP Route Flap Damping
RFC2796, BGP Route Reflection - An Alternative to Full Mesh IBGP
RFC2842, Capabilities Advertisement with BGP-4
RFC2918, Route Refresh Capability for BGP-4
RFC3065, Autonomous System Confederations for BGP

(C) 2004 - 2008 アライドテレシスホールディングス株式会社

PN: J613-M0021-12 Rev.L