[index] CentreCOM 8948XL コマンドリファレンス 2.9

# SET SNMP LOCAL

カテゴリー：運用・管理 / SNMP

`SET SNMP LOCAL={NONE|1..15} [VERSION={V1|V2|V3|ALL}]`

（SNMPv1/v2c/3）SNMPメッセージの送信に使うローカルIPインターフェース（ループバックインターフェース）を指定する。

パラメーター

LOCAL: SNMPパケットの送信に使用するローカルIPインターフェースの番号。ローカルIPインターフェースを指定した場合、SNMPパケットの始点IPアドレスとして、指定したローカルIPインターフェースのIPアドレスが使用される。省略時はNONE（ローカルIPインターフェースを使用しない。この場合、SNMPパケットの始点IPアドレスはシステムが決める）。

VERSION: 対象となるSNMPのバージョン。省略時はALL（すべてのバージョンが対象）。

関連コマンド

ADD IP LOCAL
ENABLE SNMP
SET IP LOCAL
SHOW IP INTERFACE
SHOW SNMP

参考

RFC1157, A Simple Network Management Protocol (SNMP)
RFC1213, Management Information Base for Network Management of TCP/IP-based internets: MIB-II
RFC1901, Introduction to Community-based SNMPv2
RFC1902, Structure of Management Information for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1903, Textual Conventions for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1904, Conformance Statements for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1905, Protocol Operations for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1906, Transport Mappings for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1907, Management Information Base for Version 2 of the Simple Network Management Protocol (SNMPv2)

(C) 2004 - 2008 アライドテレシスホールディングス株式会社

PN: J613-M0021-12 Rev.L