[index] CentreCOM x230/x230Lシリーズ コマンドリファレンス 5.4.8

# show spanning-tree mst

モード: 非特権EXECモード
カテゴリー: L2スイッチング / スパニングツリープロトコル

`> show spanning-tree mst [detail] [interface IFNAME]`

（MSTP）CIST（インスタンス0）の全般的な情報を表示する。さらに、オプションの組み合わせにより、インスタンス・VLAN・ポートの関連付け情報、CISTにおける各スイッチポートの情報、MSTインスタンスにおける各スイッチポートの情報などを表示する。

### パラメーター

`detail` | インスタンス・VLAN・ポートの関連付け情報ではなく、各スイッチポートの情報を表示したいときに指定する。同時にinterfaceパラメーターも指定したときは、CISTとMSTインスタンスにおける指定ポートの情報を表示する。interfaceパラメーターを指定しなかったときは、CISTにおける全ポートの情報を表示する
`interface IFNAME` | スイッチポートのインターフェース名。detailオプションと同時に指定したときは、CISTと所属先MSTインスタンスにおける指定ポートの情報を表示する。detailオプションなしで本パラメーターだけを指定したときは、インスタンス・VLAN・ポートの関連付け情報のうち、指定ポートに関連する部分だけを表示する。本パラメーター省略時は、CISTにおける全ポートの情報（detailオプションありの場合）、あるいは、すべてのインスタンス・VLAN・ポートの関連付け情報（detailオプションなしの場合）を表示する

### 使用例

    awplus> show spanning-tree mst ↓
    % 1: Bridge up - Spanning Tree Enabled
    % 1: CIST Root Path Cost 20000 - CIST Root Port 5002 -  CIST Bridge Priority 327
    68
    % 1: Forward Delay 15 - Hello Time 2 - Max Age 20 - Max-hops 20
    % 1: CIST Root Id 80000000cd08170c
    % 1: CIST Reg Root Id 80000000cd240367
    % 1: CIST Bridge Id 80000000cd240367
    % 1: CIST 2 topology changes - last topology change Mon Jan 30 06:10:23 2012
    % 1: portfast bpdu-filter disabled
    % 1: portfast bpdu-guard disabled
    % 1: portfast errdisable timeout disabled
    % 1: portfast errdisable timeout interval 300 sec
    %
    %   Instance        VLAN
    %   0:              1, 50
    %   1:              10, 20  (port1.0.11)
    %   1:              10, 20  (port1.0.10)
    %   1:              10, 20  (port1.0.12)
    %   1:              10, 20  (port1.0.3)
    %   2:              30, 40  (port1.0.11)
    %   2:              30, 40  (port1.0.1)
    %   2:              30, 40  (port1.0.5)
    %   2:              30, 40  (port1.0.7)

    awplus> show spanning-tree mst detail ↓
    % 1: Bridge up - Spanning Tree Enabled
    % 1: CIST Root Path Cost 20000 - CIST Root Port 5002 -  CIST Bridge Priority 327
    68
    % 1: Forward Delay 15 - Hello Time 2 - Max Age 20 - Max-hops 20
    % 1: CIST Root Id 80000000cd08170c
    % 1: CIST Reg Root Id 80000000cd240367
    % 1: CIST Bridge Id 80000000cd240367
    % 1: CIST 2 topology changes - last topology change Mon Jan 30 06:10:23 2012
    % 1: portfast bpdu-filter disabled
    % 1: portfast bpdu-guard disabled
    % 1: portfast errdisable timeout disabled
    % 1: portfast errdisable timeout interval 300 sec
    %   port1.0.1: Port 5001 - Id 8389 - Role Designated - State Forwarding
    %   port1.0.1: Designated External Path Cost 20000 -Internal Path Cost 0
    %   port1.0.1: Configured Path Cost 200000  - Add type Explicit ref count 1
    %   port1.0.1: Designated Port Id 8389 - CIST Priority 128  -
    %   port1.0.1: CIST Root 80000000cd08170c
    %   port1.0.1: Regional Root 80000000cd240367
    %   port1.0.1: Designated Bridge 80000000cd240367
    %   port1.0.1: Message Age 1 - Max Age 20
    %   port1.0.1: CIST Hello Time 2 - Forward Delay 15
    %   port1.0.1: CIST Forward Timer 0 - Msg Age Timer 0 - Hello Timer 0 - topo cha
    nge timer 0
    %   port1.0.1: forward-transitions 3
    %   port1.0.1: Version Multiple Spanning Tree Protocol - Received RSTP - Send MS
    TP
    %   port1.0.1: No portfast configured - Current  portfast off
    %   port1.0.1: portfast bpdu-guard  default  - Current portfast bpdu-guard off
    %   port1.0.1: portfast bpdu-filter default  - Current portfast bpdu-filter off
    %   port1.0.1: no root guard configured     - Current root guard off
    %   port1.0.1: Configured Link Type point-to-point - Current point-to-point
    %
    %   port1.0.2: Port 5002 - Id 838a - Role Rootport - State Forwarding
    ...

    awplus> show spanning-tree mst interface port1.0.11 ↓
    % 1: Bridge up - Spanning Tree Enabled
    % 1: CIST Root Path Cost 20000 - CIST Root Port 5002 -  CIST Bridge Priority 327
    68
    % 1: Forward Delay 15 - Hello Time 2 - Max Age 20 - Max-hops 20
    % 1: CIST Root Id 80000000cd08170c
    % 1: CIST Reg Root Id 80000000cd240367
    % 1: CIST Bridge Id 80000000cd240367
    % 1: CIST 2 topology changes - last topology change Mon Jan 30 06:10:23 2012
    % 1: portfast bpdu-filter disabled
    % 1: portfast bpdu-guard disabled
    % 1: portfast errdisable timeout disabled
    % 1: portfast errdisable timeout interval 300 sec
    %
    %   Instance        VLAN
    %   0:              1, 50
    %   1:              10, 20  (port1.0.11)
    %   2:              30, 40  (port1.0.11)

    awplus> show spanning-tree mst detail interface port1.0.1 ↓
    % 1: Bridge up - Spanning Tree Enabled
    % 1: CIST Root Path Cost 0 - CIST Root Port 0 -  CIST Bridge Priority 32768
    % 1: Forward Delay 15 - Hello Time 2 - Max Age 20 - Max-hops 20
    % 1: CIST Root Id 80000000cd240367
    % 1: CIST Reg Root Id 80000000cd240367
    % 1: CIST Bridge Id 80000000cd240367
    % 1: CIST 2 topology changes - last topology change Mon Jan 30 06:10:23 2012
    % 1: portfast bpdu-filter disabled
    % 1: portfast bpdu-guard disabled
    % 1: portfast errdisable timeout disabled
    % 1: portfast errdisable timeout interval 300 sec
    %   port1.0.1: Port 5001 - Id 8389 - Role Designated - State Forwarding
    %   port1.0.1: Designated External Path Cost 0 -Internal Path Cost 0
    %   port1.0.1: Configured Path Cost 200000  - Add type Explicit ref count 3
    %   port1.0.1: Designated Port Id 8389 - CIST Priority 128  -
    %   port1.0.1: CIST Root 80000000cd240367
    %   port1.0.1: Regional Root 80000000cd240367
    %   port1.0.1: Designated Bridge 80000000cd240367
    %   port1.0.1: Message Age 0 - Max Age 20
    %   port1.0.1: CIST Hello Time 2 - Forward Delay 15
    %   port1.0.1: CIST Forward Timer 0 - Msg Age Timer 0 - Hello Timer 1 - topo cha
    nge timer 0
    %   port1.0.1: forward-transitions 3
    %   port1.0.1: Version Multiple Spanning Tree Protocol - Received MSTP - Send MS
    TP
    %   port1.0.1: No portfast configured - Current  portfast off
    %   port1.0.1: portfast bpdu-guard  default  - Current portfast bpdu-guard off
    %   port1.0.1: portfast bpdu-filter default  - Current portfast bpdu-filter off
    %   port1.0.1: no root guard configured     - Current root guard off
    %   port1.0.1: Configured Link Type point-to-point - Current point-to-point
    %
    % Instance  1:  Vlans: 10
    % 1: MSTI Root Path Cost 0 -MSTI Root Port 0 - MSTI Bridge Priority 4096
    % 1: MSTI Root Id 10010000cd240367
    % 1: MSTI Bridge Id 10010000cd240367
    %   port1.0.1: Port 5001 - Id 8389 - Role Designated - State Forwarding
    %   port1.0.1: Designated Internal Path Cost 0  - Designated Port Id 8389
    %   port1.0.1: Configured Internal Path Cost 200000
    %   port1.0.1: Configured CST External Path cost 200000
    %   port1.0.1: CST Priority 128  - MSTI Priority 128
    %   port1.0.1: Designated Root 10010000cd240367
    %   port1.0.1: Designated Bridge 10010000cd240367
    %   port1.0.1: Message Age 0 - Max Age 0
    %   port1.0.1: Hello Time 2 - Forward Delay 15
    %   port1.0.1: Forward Timer 0 - Msg Age Timer 0 - Hello Timer 1

    % Instance  2:  Vlans: 20
    % 1: MSTI Root Path Cost 2000 -MSTI Root Port 5002 - MSTI Bridge Priority 8192
    % 1: MSTI Root Id 10020000f4272c74
    % 1: MSTI Bridge Id 20020000cd240367
    %   port1.0.1: Port 5001 - Id 8389 - Role Alternate - State Discarding
    %   port1.0.1: Designated Internal Path Cost 0  - Designated Port Id 8389
    %   port1.0.1: Configured Internal Path Cost 200000
    %   port1.0.1: Configured CST External Path cost 200000
    %   port1.0.1: CST Priority 128  - MSTI Priority 128
    %   port1.0.1: Designated Root 10020000f4272c74
    %   port1.0.1: Designated Bridge 10020000f4272c74
    %   port1.0.1: Message Age 0 - Max Age 0
    %   port1.0.1: Hello Time 2 - Forward Delay 15
    %   port1.0.1: Forward Timer 0 - Msg Age Timer 4 - Hello Timer 1

表 1
Bridge up | スパニングツリープロトコルの有効/無効
CIST Root Path Cost | ルートブリッジのパスコスト
CIST Root Port | ルートポートのインターフェースインデックス番号。ルートブリッジのときは 0 と表示される。トランクポートの場合はトランクグループのインターフェースインデックス番号で表示される
CIST Bridge Priority | ブリッジプライオリティー
Forward Delay | ルートブリッジのフォワードディレイタイム設定値
Hello Time | ルートブリッジのハロータイム設定値
Max Age | ルートブリッジの最大エージタイム設定値
Max-hops | 最大ホップ数 設定値
CIST Root Id | ルートのブリッジ識別子。ルートのブリッジプライオリティー（16進数先頭4桁）とMACアドレスで構成される
CIST Reg Root Id | リージョンのRoot ID
CIST Bridge Id | ブリッジ識別子。ブリッジプライオリティー（16進数先頭4桁）とMACアドレスで構成される
CIST topology change(s) | トポロジーチェンジが発生した回数（厳密にはTCフラグの付いたBPDUの数を示す）
last topology change | 最後にトポロジーチェンジが発生した日時
portfast bpdu-filter | BPDUフィルター機能の有効/無効
portfast bpdu-guard | BPDUガード機能の有効/無効
portfast errdisable timeout | BPDUガード機能によって無効化されたエッジポートを、一定時間後に自動的に再有効化する機能の有効/無効
portfast errdisable timeout interval | BPDUガード機能によって無効化されたエッジポートを、自動的に再有効化するまでの待機時間

### 注意・補足事項

■ 本コマンドを実行しても、スパニングツリープロトコルの動作モードがMSTPでない場合は何も表示されない。
■ 本コマンドはEXECモードだけでなくインターフェースモードでも実行できる。

### 関連コマンド

instance vlan（MSTモード）
spanning-tree mode（グローバルコンフィグモード）
spanning-tree mst instance（インターフェースモード）

(C) 2014 - 2018 アライドテレシスホールディングス株式会社

PN: 613-001990 Rev.T