[index] CentreCOM IE340/IE340L シリーズ コマンドリファレンス 5.5.4

# show ipv6 prefix-list

モード: 特権EXECモード
カテゴリー: IP / 経路制御（フィルタリング）

`# show ipv6 prefix-list PLISTNAME`

`# show ipv6 prefix-list [detail|summary] [PLISTNAME]`

IPv6プレフィックスリストを表示する。

### パラメーター

`PLISTNAME` | IPv6プレフィックスリスト名
`detail` | 詳細情報を表示させたいときに指定する
`summary` | サマリー情報を表示させたいときに指定する

### 使用例

■ オプション無指定時

    awplus# show ipv6 prefix-list ↓
    ipv6 prefix-list p1: 2 entries
         seq 5 deny 2001:db8:10::/48 le 64
         seq 10 permit any
    ipv6 prefix-list p3: 2 entries
         seq 5 deny 2001:db8:3c:10::/64
         seq 10 permit any

■ summaryオプション指定時

    awplus# show ipv6 prefix-list summary ↓
    Prefix-list with the last deletion/insertion: p3
    ipv6 prefix-list p1:
       count: 2, range entries: 0, sequences: 5 - 10
    ipv6 prefix-list p3:
       count: 2, range entries: 0, sequences: 5 - 10

■ detailオプション指定時

    awplus# show ipv6 prefix-list detail ↓
    Prefix-list with the last deletion/insertion: p3
    ipv6 prefix-list p1:
       count: 2, range entries: 0, sequences: 5 - 10
        ripd:
         seq 5 deny 2001:db8:10::/48 le 64 (hit count: 0, refcount: 0)
         seq 10 permit any (hit count: 0, refcount: 0)
        ripngd:
         seq 5 deny 2001:db8:10::/48 le 64 (hit count: 0, refcount: 0)
         seq 10 permit any (hit count: 0, refcount: 0)
        ospfd:
         seq 5 deny 2001:db8:10::/48 le 64 (hit count: 0, refcount: 0)
         seq 10 permit any (hit count: 0, refcount: 0)
        bgpd:
         seq 5 deny 2001:db8:10::/48 le 64 (hit count: 0, refcount: 0)
         seq 10 permit any (hit count: 0, refcount: 0)
    ipv6 prefix-list p3:
       count: 2, range entries: 0, sequences: 5 - 10
        ripd:
         seq 5 deny 2001:db8:3c:10::/64 (hit count: 0, refcount: 0)
         seq 10 permit any (hit count: 0, refcount: 0)
        ripngd:
         seq 5 deny 2001:db8:3c:10::/64 (hit count: 0, refcount: 0)
         seq 10 permit any (hit count: 0, refcount: 0)
        ospfd:
         seq 5 deny 2001:db8:3c:10::/64 (hit count: 0, refcount: 0)
         seq 10 permit any (hit count: 0, refcount: 0)
        bgpd:
         seq 5 deny 2001:db8:3c:10::/64 (hit count: 0, refcount: 0)
         seq 10 permit any (hit count: 0, refcount: 0)

### 関連コマンド

clear ipv6 prefix-list（特権EXECモード）
ipv6 prefix-list（グローバルコンフィグモード）

(C) 2019 - 2025 アライドテレシスホールディングス株式会社

PN: 613-002778 Rev.AA