[index] CentreCOM IE340/IE340L シリーズ コマンドリファレンス 5.5.4

# show counter mrp

モード: 特権EXECモード
カテゴリー: L2スイッチング / MRP

`# show counter mrp [global | ring <1-65535>]`

MRPリングの統計カウンターを表示する。

### パラメーター

`global` | グローバルMRPカウンターのみを無効にする
`ring <1-65535>` | MRPリングIDのカウンターのみを表示する

### 使用例

    awplus# show counter mrp ↓
    Media Redundancy Protocol Global Counters

    MRP Started             ....... 2
    MRP Dispatcher          ....... 19102219
    MRP Timer Tick          ....... 17373917
    MRP Packet RX           ....... 1728302
    MRP Packet RX Error     ....... 0
    MRP Packet TX           ....... 1728303
    MRP Packet TX Error     ....... 0

    Media Redundancy Protocol Ring 1 Counters

    Port 1 PDUs Received
    MRP_Test              ......... 864150
    MRP_TopologyChange    ......... 0
    MRP_LinkUp            ......... 0
    MRP_LinkDown          ......... 0

    Port 1 PDUs Transferred
    MRP_Test              ......... 864152
    MRP_TopologyChange    ......... 0
    MRP_LinkUp            ......... 0
    MRP_LinkDown          ......... 0

    Port 2 PDUs Received
    MRP_Test              ......... 864152
    MRP_TopologyChange    ......... 0
    MRP_LinkUp            ......... 0
    MRP_LinkDown          ......... 0

    Port 2 PDUs Transferred
    MRP_Test              ......... 864152
    MRP_TopologyChange    ......... 0
    MRP_LinkUp            ......... 0
    MRP_LinkDown          ......... 0

    Other Counters
    State Changes         ......... 6
    Port Blocked Set      ......... 4
    Port Forwarding Set   ......... 2

    awplus# show counter mrp global ↓
    Media Redundancy Protocol Global Counters

    MRP Started             ....... 2
    MRP Dispatcher          ....... 19211403
    MRP Timer Tick          ....... 17473175
    MRP Packet RX           ....... 1738228
    MRP Packet RX Error     ....... 0
    MRP Packet TX           ....... 1738229
    MRP Packet TX Error     ....... 0

    awplus# show counter mrp ring 1 ↓
    Media Redundancy Protocol Ring 1 Counters

    Port 1 PDUs Received
    MRP_Test              ......... 871675
    MRP_TopologyChange    ......... 0
    MRP_LinkUp            ......... 0
    MRP_LinkDown          ......... 0

    Port 1 PDUs Transferred
    MRP_Test              ......... 871677
    MRP_TopologyChange    ......... 0
    MRP_LinkUp            ......... 0
    MRP_LinkDown          ......... 0

    Port 2 PDUs Received
    MRP_Test              ......... 871677
    MRP_TopologyChange    ......... 0
    MRP_LinkUp            ......... 0
    MRP_LinkDown          ......... 0

    Port 2 PDUs Transferred
    MRP_Test              ......... 871677
    MRP_TopologyChange    ......... 0
    MRP_LinkUp            ......... 0
    MRP_LinkDown          ......... 0

    Other Counters
    State Changes         ......... 6
    Port Blocked Set      ......... 4
    Port Forwarding Set   ......... 2

### 関連コマンド

service mrp（グローバルコンフィグモード）
mrp ring（インターフェースモード）
domain-name（MRPリングモード）
vlan-id（MRPリングモード）
profile（MRPリングモード）
role（MRPリングモード）
lc-react（MRPリングマネージャーモード）
enable（MRPリングモード）
mrp ring（グローバルコンフィグモード）
show mrp ring（特権EXECモード）
clear counter mrp（特権EXECモード）

(C) 2019 - 2025 アライドテレシスホールディングス株式会社

PN: 613-002778 Rev.AA