[index] CentreCOM x240シリーズ コマンドリファレンス 5.5.5

# show auth supplicant

モード: 特権EXECモード
カテゴリー: インターフェース / ポート認証

`# show auth supplicant [interface IFRANGE] [brief]`

`# show auth [interface IFRANGE] supplicant [brief]`

各スイッチポートにおけるポート認証のSupplicant情報を表示する。

### パラメーター

`interface IFRANGE` | スイッチポートのインターフェース名。指定したスイッチポートの情報だけを表示させたいときに指定する。ハイフン、カンマを使った複数指定も可能。省略時はすべてのインターフェースが対象となる
`brief` | Supplicantの情報を簡素な形式で表示する

### 使用例

    awplus# show auth supplicant ↓
    Interface port1.0.1
      authenticationMethod: mac
      totalSupplicantNum: 1
      authorizedSupplicantNum: 1
        macBasedAuthenticationSupplicantNum: 1
        dot1xAuthenticationSupplicantNum: 0
        webBasedAuthenticationSupplicantNum: 0
        otherAuthenticationSupplicantNum: 0

      Supplicant name: 00-13-3b-0c-6c-2b
      Supplicant address: 0013.3b0c.6c2b
        authenticationMethod: MAC-based Authentication
        portStatus: Authorized - currentId: 1
        abort:F fail:F start:F timeout:F success:T
        PAE: state: Authenticated - portMode: Auto
        PAE: reAuthCount: 0 - rxRespId: 0
        PAE: quietPeriod: 60 - maxReauthReq: 2
        BE: state: Idle - reqCount: 0 - idFromServer: 0
        CD: adminControlledDirections: in - operControlledDirections: in
        CD: bridgeDetected: false
        KR: rxKey: false
        KT: keyAvailable: false - keyTxEnabled: false
        RADIUS server group (auth): radius
        RADIUS server (auth): 192.168.1.5

    awplus# show auth supplicant brief ↓
    Interface port1.0.1
      authenticationMethod: mac
      totalSupplicantNum: 1
      authorizedSupplicantNum: 1
        macBasedAuthenticationSupplicantNum: 1
        dot1xAuthenticationSupplicantNum: 0
        webBasedAuthenticationSupplicantNum: 0
        otherAuthenticationSupplicantNum: 0

    Interface   VID  Mode MAC Address    Status            IP Address      Username
    =========== ==== ==== ============== ================= =============== ========
    port1.0.1   1    M    0013.3b0c.6c2b Authenticated     --              00-13...

    awplus# show auth supplicant interface port1.0.1 ↓
    Interface port1.0.1
      authenticationMethod: mac
      totalSupplicantNum: 1
      authorizedSupplicantNum: 1
        macBasedAuthenticationSupplicantNum: 1
        dot1xAuthenticationSupplicantNum: 0
        webBasedAuthenticationSupplicantNum: 0
        otherAuthenticationSupplicantNum: 0

      Supplicant name: 00-13-3b-0c-6c-2b
      Supplicant address: 0013.3b0c.6c2b
        authenticationMethod: MAC-based Authentication

    awplus# show auth supplicant interface port1.0.1 brief ↓
    Interface port1.0.1
      authenticationMethod: mac
      totalSupplicantNum: 1
      authorizedSupplicantNum: 1
        macBasedAuthenticationSupplicantNum: 1
        dot1xAuthenticationSupplicantNum: 0
        webBasedAuthenticationSupplicantNum: 0
        otherAuthenticationSupplicantNum: 0

    Interface   VID  Mode MAC Address    Status            IP Address      Username
    =========== ==== ==== ============== ================= =============== ========
    port1.0.1   1    M    0013.3b0c.6c2b Authenticated     --              00-13...

### 注意・補足事項

■ 実際には他の認証方式のSupplicant情報も表示されるが、briefオプションなしで実行した場合、他の認証方式のSupplicantの情報は簡潔に表示される。

### 関連コマンド

aaa authentication auth-mac（グローバルコンフィグモード）
auth dynamic-acl enable（インターフェースモード）
auth two-step enable（インターフェースモード）
auth-mac enable（インターフェースモード）
auth-web enable（インターフェースモード）
show dot1x supplicant（特権EXECモード）

(C) 2023 - 2025 アライドテレシスホールディングス株式会社

PN: 613-003248 Rev.M