[index] CentreCOM x930シリーズ コマンドリファレンス 5.5.5

# show ipv6 ospf interface

モード: 非特権EXECモード
カテゴリー: IPv6 / 経路制御（OSPFv3）

`> show ipv6 ospf interface [IFNAME]`

OSPFv3インターフェースの情報を表示する。

### パラメーター

`IFNAME` | インターフェース名。省略時はすべてのOSPFv3インターフェースが対象となる

### 使用例

    awplus> show ipv6 ospf interface ↓
    vlan1 is up, line protocol is up
      Interface ID 301
      IPv6 Prefixes
        fe80::200:cdff:fe28:748/64 (Link-Local Address)
        2001:db8:2222:10::5/64
      Security Policy
        Authentication NULL
        Encryption NULL

      OSPFv3 Process (*null*), Area 0.0.0.0, Instance ID 0
        Router ID 10.10.10.5, Network Type BROADCAST, Cost: 1
        Transmit Delay is 1 sec, State DR, Priority 1
        Interface state DR
        Designated Router (ID) 10.10.10.5
          Interface Address fe80::200:cdff:fe28:748
        Backup Designated Router (ID) 10.10.10.1
          Interface Address fe80::200:cdff:fe28:747
        Timer interval configured, Hello 10, Dead 40, Wait 40, Retransmit 5
          Hello due in 00:00:08
        Neighbor Count is 1, Adjacent neighbor count is 1
    vlan10 is up, line protocol is up
      Interface ID 310
      IPv6 Prefixes
        fe80::200:cdff:fe28:748/64 (Link-Local Address)
        2001:db8:5000:10::1/64

      OSPFv3 Process (*null*), Area 0.0.0.2, Instance ID 0
        Router ID 10.10.10.5, Network Type BROADCAST, Cost: 1
        Transmit Delay is 1 sec, State DR, Priority 1
        Interface state DR
        Designated Router (ID) 10.10.10.5
          Interface Address fe80::200:cdff:fe28:748
        No backup designated router on this link
        Timer interval configured, Hello 10, Dead 40, Wait 40, Retransmit 5
          Hello due in 00:00:05
        Neighbor Count is 0, Adjacent neighbor count is 0

### 注意・補足事項

■ 本機能の設定を行う際は、あらかじめOSPF6サービスを有効にしておくこと（service ospf6コマンド）。

(C) 2015 - 2025 アライドテレシスホールディングス株式会社

PN: 613-002105 Rev.AZ