[index] SwitchBlade x908 GEN2 コマンドリファレンス 5.5.5

# show macsec

モード: 特権EXECモード
カテゴリー: L2スイッチング / MACsec

`# show macsec [interface IFRANGE]`

MACsecが有効なポートの全般的情報を表示する。

### パラメーター

`interface IFRANGE` | インターフェース名。ハイフン、カンマを使った複数指定も可能。省略時はMACsecが有効なすべてのインターフェースが対象となる

### 使用例

    awplus# show macsec interface port1.1.5 ↓

    MKA and MACsec information for interface port1.1.5:

      MKA:

        Pre-shared CAK Size (Bits):    256

        Active:                        True
        Actor SCI:                     e01a.ea2a.4f49/13f1
        Actor Priority:                128
        Key Server SCI:                e01a.ea2a.4f49/13f1
        Key Server Priority:           128
        Keys Distributed:              1
        Keys Received:                 0

        MACsec Settings Received:      True
        MACsec Settings Accepted:      True
        MACsec Cipher Suite:           GCM-AES-128
        MACsec Protection Mode:        Integrity and confidentiality

      General MACsec Info:

        Hardware Ready:                True
        Current Cipher Suite:          GCM-AES-128
        Cipher Suite Protection:       Integrity and confidentiality

        Input Data Pkts (Allowed):     3
        Input Data Pkts (Blocked):     0
        Input EAPOL Pkts:              2

        Output Data Pkts (OK):         5
        Output Data Pkts (Error):      0
        Output EAPOL Pkts:             6

      Frame Generation:

        Protect Frames:                True
        Always Include SCI:            True

        Pkts Untagged:                 0
        Pkts Too Long:                 0

        Bytes Protected Only:          0
        Bytes Encrypted:               240

      Frame Verification:

        Validate Frames:               Strict
        Replay Protect:                True
        Replay Window:                 0

        Pkts Untagged (Allowed):       0
        Pkts Untagged (Blocked):       0
        Pkts Bad Tag:                  0
        Pkts Unknown SCI (Allowed):    0
        Pkts Unknown SCI (Blocked):    0
        Pkts Overrun:                  0

        Bytes Validated Only:          0
        Bytes Decrypted:               144

      Transmit Channel e01a.ea2a.4f49/13f1:

        Created Time:                  2021-11-26 17:05:55

        Pkts Protected Only:           0
        Pkts Encrypted:                5

        Secure Association 0:

          Key Identifier:              913E1BEA38E05A53120AB44500000001
          Created Time:                2021-11-26 17:06:02
          In Use:                      True
          Next Packet Number:          0x00000006

          Pkts Protected Only:         0
          Pkts Encrypted:              5

      Receive Channel 0800.2775.c06d/0001:

        Created Time:                  2021-11-26 17:06:00

        Pkts OK:                       3
        Pkts Unchecked:                0
        Pkts Invalid (Allowed):        0
        Pkts Invalid (Blocked):        0
        Pkts Late (Allowed):           0
        Pkts Late (Blocked):           0

        Secure Association 0:

          Key Identifier:              913E1BEA38E05A53120AB44500000001
          Created Time:                2021-11-26 17:06:02
          In Use:                      True
          Next Packet Number:          0x00000004

          Pkts OK:                     3
          Pkts Invalid (Allowed):      0
          Pkts Invalid (Blocked):      0

### 関連コマンド

clear macsec counters（特権EXECモード）
mka policy（グローバルコンフィグモード）
mka policy（インターフェースモード）
show mka policy（特権EXECモード）

(C) 2017 - 2025 アライドテレシスホールディングス株式会社

PN: 613-002489 Rev.AP