[index] SwitchBlade x908 GEN2 コマンドリファレンス 5.5.5

# show system environment

モード: 非特権EXECモード
カテゴリー: 運用・管理 / システム

`> show system environment`

本体、拡張モジュール、電源ユニット/ファンモジュールの動作環境に関する情報を表示する。

### 使用例

    awplus> show system environment ↓
    Environment Monitoring Status

    Stack member 1:

    Overall Status: Normal

    Resource ID: 9  Name: PSU Bay A ()
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                           No        -          -       Ok
    2   Fault                                    No        -          -       Ok
    3   PSU Power Output                         No        -          -       Ok
    4   PSU Power Input                          No        -          -       Ok

    Resource ID: 10  Name: PSU Bay B (AT-SBxPWRSYS2/AC)
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                          Yes        -          -       Ok
    2   Fault                                    No        -          -       Ok
    3   PSU Power Output                        Yes        -          -       Ok
    4   PSU Power Input                         Yes        -          -       Ok

    Resource ID: 11  Name: Fan Tray A (AT-FAN08)
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                          Yes        -          -       Ok

    Resource ID: 12  Name: Fan Tray B (AT-FAN08)
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                          Yes        -          -       Ok

    Resource ID: 100  Name: AT-SBx908 GEN2
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Voltage: 2.5V (Volts)                 2.487      2.344      2.865     Ok
    2   Voltage: Battery (Volts)              3.150      2.700      3.586     Ok
    3   Voltage: 3.3V (Volts)                 3.300      2.973      3.627     Ok
    4   Voltage: 12.0V (Volts)               12.125     10.813     13.188     Ok
    5   Voltage: 1.0V (Volts)                 0.998      0.900      1.097     Ok
    6   Temp: Internal (Degrees C)               34   70(Hyst)         75     Ok
    7   Temp: Fan Tray A 1 (Degrees C)           31         -5         70     Ok
    8   Temp: Fan Tray A 2 (Degrees C)           29         -5         70     Ok
    9   Temp: Fan Tray B 1 (Degrees C)           30         -5         70     Ok
    10  Temp: Fan Tray B 2 (Degrees C)           31         -5         70     Ok
    11  Temp: Near Switch (Degrees C)            34   70(Hyst)         75     Ok
    12  Temp: Front Left (Degrees C)             30   65(Hyst)         70     Ok
    13  Temp: Front Mid (Degrees C)              29   65(Hyst)         70     Ok
    14  Temp: Front Right (Degrees C)            30   65(Hyst)         70     Ok
    15  Temp: Console (Degrees C)                32   55(Hyst)         60     Ok

    Resource ID: 101  Name: AT-XEM2-12XT  Bay: 1
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Temp: XEM Front (Degrees C)              29   55(Hyst)         60     Ok
    2   Temp: XEM Rear (Degrees C)               37   70(Hyst)         75     Ok

    Resource ID: 111  Name: AT-FAN08
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Fan:  Fan Tray A 1 Int (Rpm)           4072       3000        -       Ok
    2   Fan:  Fan Tray A 1 Ext (Rpm)           3651       3000        -       Ok
    3   Fan:  Fan Tray A 2 Int (Rpm)           3997       3000        -       Ok
    4   Fan:  Fan Tray A 2 Ext (Rpm)           3624       3000        -       Ok

    Resource ID: 112  Name: AT-FAN08
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Fan:  Fan Tray B 1 Int (Rpm)           4215       3000        -       Ok
    2   Fan:  Fan Tray B 1 Ext (Rpm)           3846       3000        -       Ok
    3   Fan:  Fan Tray B 2 Int (Rpm)           4238       3000        -       Ok
    4   Fan:  Fan Tray B 2 Ext (Rpm)           3629       3000        -       Ok

    ...

> Note

> > 上記表示は一例です。表示される内容は製品、バージョン、機器構成などによって異なります。

### 注意・補足事項

■ VCSマスターに対して本コマンドを実行した場合は、すべてのスタックメンバーに関する情報を表示する。

### 関連コマンド

show system（非特権EXECモード）
show system pluggable（非特権EXECモード）

(C) 2017 - 2025 アライドテレシスホールディングス株式会社

PN: 613-002489 Rev.AP