[index] CentreCOM x950シリーズ コマンドリファレンス 5.5.5

# show spanning-tree

モード: 非特権EXECモード
カテゴリー: L2スイッチング / スパニングツリープロトコル

`> show spanning-tree [interface IFRANGE]`

スパニングツリープロトコルの全般的な情報、および、各スイッチポートのスパニングツリー関連情報を表示する。

### パラメーター

`interface IFRANGE` | スイッチポートのインターフェース名。ハイフン、カンマを使った複数指定も可能。省略時はすべてのポートが対象となる

### 使用例

■ スパニングツリープロトコルの全般的な情報と全スイッチポートのスパニングツリー関連情報を表示する。

    awplus> show spanning-tree ↓
    % 1: Bridge up - Spanning Tree Enabled
    % 1: Root Path Cost 20000 - Root Port 5002 -  Bridge Priority 32768
    % 1: Forward Delay 15 - Hello Time 2 - Max Age 20
    % 1: Root Id 80000000cd08170c
    % 1: Bridge Id 80000000cd240367
    % 1: 2 topology changes - last topology change Mon Jan 31 06:05:37 2012
    % 1: portfast bpdu-filter disabled
    % 1: portfast bpdu-guard disabled
    % 1: portfast errdisable timeout disabled
    % 1: portfast errdisable timeout interval 300 sec
    %   port1.0.1: Port 5001 - Id 8389 - Role Designated - State Forwarding
    %   port1.0.1: Designated Path Cost 20000
    %   port1.0.1: Configured Path Cost 200000  - Add type Explicit ref count 1
    %   port1.0.1: Designated Port Id 8389 - Priority 128  -
    %   port1.0.1: Root 80000000cd08170c
    %   port1.0.1: Designated Bridge 80000000cd240367
    %   port1.0.1: Message Age 1 - Max Age 20
    %   port1.0.1: Hello Time 2 - Forward Delay 15
    %   port1.0.1: Forward Timer 0 - Msg Age Timer 0 - Hello Timer 0 - topo change t
    imer 0
    %   port1.0.1: forward-transitions 6
    %   port1.0.1: Version Rapid Spanning Tree Protocol - Received RSTP - Send RSTP
    %   port1.0.1: No portfast configured - Current  portfast off
    %   port1.0.1: portfast bpdu-guard  default  - Current portfast bpdu-guard off
    %   port1.0.1: portfast bpdu-filter default  - Current portfast bpdu-filter off
    %   port1.0.1: no root guard configured     - Current root guard off
    %   port1.0.1: Configured Link Type point-to-point - Current point-to-point
    %
    %   port1.0.2: Port 5002 - Id 838a - Role Rootport - State Forwarding
    ...

■ スパニングツリープロトコルの全般的な情報とスイッチポート1.0.1～1.0.2のスパニングツリー関連情報を表示する。

    awplus> show spanning-tree interface port1.0.1-1.0.2 ↓
    % 1: Bridge up - Spanning Tree Enabled
    % 1: Root Path Cost 20000 - Root Port 5002 -  Bridge Priority 32768
    % 1: Forward Delay 15 - Hello Time 2 - Max Age 20
    % 1: Root Id 80000000cd08170c
    % 1: Bridge Id 80000000cd240367
    % 1: 2 topology changes - last topology change Mon Jan 30 06:05:37 2012
    % 1: portfast bpdu-filter disabled
    % 1: portfast bpdu-guard disabled
    % 1: portfast errdisable timeout disabled
    % 1: portfast errdisable timeout interval 300 sec
    %   port1.0.1: Port 5001 - Id 8389 - Role Designated - State Forwarding
    %   port1.0.1: Designated Path Cost 20000
    %   port1.0.1: Configured Path Cost 200000  - Add type Explicit ref count 1
    %   port1.0.1: Designated Port Id 8389 - Priority 128  -
    %   port1.0.1: Root 80000000cd08170c
    %   port1.0.1: Designated Bridge 80000000cd240367
    %   port1.0.1: Message Age 1 - Max Age 20
    %   port1.0.1: Hello Time 2 - Forward Delay 15
    %   port1.0.1: Forward Timer 0 - Msg Age Timer 0 - Hello Timer 0 - topo change t
    imer 0
    %   port1.0.1: forward-transitions 6
    %   port1.0.1: Version Rapid Spanning Tree Protocol - Received RSTP - Send RSTP
    %   port1.0.1: No portfast configured - Current  portfast off
    %   port1.0.1: portfast bpdu-guard  default  - Current portfast bpdu-guard off
    %   port1.0.1: portfast bpdu-filter default  - Current portfast bpdu-filter off
    %   port1.0.1: no root guard configured     - Current root guard off
    %   port1.0.1: Configured Link Type point-to-point - Current point-to-point
    %
    %
    % 1: Bridge up - Spanning Tree Enabled
    % 1: Root Path Cost 20000 - Root Port 5002 -  Bridge Priority 32768
    % 1: Forward Delay 15 - Hello Time 2 - Max Age 20
    % 1: Root Id 80000000cd08170c
    % 1: Bridge Id 80000000cd240367
    % 1: 2 topology changes - last topology change Mon Jan 30 06:05:37 2012
    % 1: portfast bpdu-filter disabled
    % 1: portfast bpdu-guard disabled
    % 1: portfast errdisable timeout disabled
    % 1: portfast errdisable timeout interval 300 sec
    %   port1.0.2: Port 5002 - Id 838a - Role Rootport - State Forwarding
    %   port1.0.2: Designated Path Cost 0
    %   port1.0.2: Configured Path Cost 20000  - Add type Explicit ref count 1
    %   port1.0.2: Designated Port Id 8002 - Priority 128  -
    %   port1.0.2: Root 80000000cd08170c
    %   port1.0.2: Designated Bridge 80000000cd08170c
    %   port1.0.2: Message Age 1 - Max Age 20
    %   port1.0.2: Hello Time 2 - Forward Delay 15
    %   port1.0.2: Forward Timer 0 - Msg Age Timer 4 - Hello Timer 1 - topo change t
    imer 0
    %   port1.0.2: forward-transitions 3
    %   port1.0.2: Version Rapid Spanning Tree Protocol - Received RSTP - Send RSTP
    %   port1.0.2: No portfast configured - Current  portfast off
    %   port1.0.2: portfast bpdu-guard  default  - Current portfast bpdu-guard off
    %   port1.0.2: portfast bpdu-filter default  - Current portfast bpdu-filter off
    %   port1.0.2: no root guard configured     - Current root guard off
    %   port1.0.2: Configured Link Type point-to-point - Current point-to-point

表 1
Bridge up | スパニングツリープロトコルの有効/無効
Root Path Cost | ルートブリッジのパスコスト
Root Port | ルートポートのインターフェースインデックス番号。ルートブリッジのときは 0 と表示される。トランクポートの場合はトランクグループのインターフェースインデックス番号で表示される
Bridge Priority | ブリッジプライオリティー
Forward Delay | ルートブリッジのフォワードディレイタイム設定値
Hello Time | ルートブリッジのハロータイム設定値
Max Age | ルートブリッジの最大エージタイム設定値
Root Id | ルートのブリッジ識別子。ルートのブリッジプライオリティー（16進数先頭4桁）とMACアドレスで構成される
Bridge Id | ブリッジ識別子。ブリッジプライオリティー（16進数先頭4桁）とMACアドレスで構成される
topology change(s) | トポロジーチェンジが発生した回数（厳密にはTCフラグの付いたBPDUの数を示す）
last topology change | 最後にトポロジーチェンジが発生した日時
portfast bpdu-filter | BPDUフィルター機能の有効/無効
portfast bpdu-guard | BPDUガード機能の有効/無効
portfast errdisable timeout | BPDUガード機能によって無効化されたエッジポートを、一定時間後に自動的に再有効化する機能の有効/無効
portfast errdisable timeout interval | BPDUガード機能によって無効化されたエッジポートを、自動的に再有効化するまでの待機時間
Ifindex | インターフェースインデックス番号
Port Id | ポートのポートID
Role | ポートの役割。Disabled、Designated、Rootport、Alternate、Backupのいずれか
State | ポートの状態。Listening、Learning、Forwarding、Discardingのいずれか
Designated Path Cost | パスコスト
Configured Path Cost | インターフェースのパスコスト設定値
Add type Explicit ref count | そのポートが所属するSTPドメインの数
Designated Port Id | DesignatedポートのID
Priority | ポートプライオリティー
Root | ルートのブリッジ識別子。ルートのブリッジプライオリティー（16進数先頭4桁）とMACアドレスで構成される
Designated Bridge | ブリッジ識別子。ブリッジプライオリティー（16進数先頭4桁）とMACアドレスで構成される
Message Age | メッセージ経過時間
Max Age | 最大エージタイム設定値
Hello Time | ハロータイム設定値
Forward Delay | フォワードディレイタイム設定値
Forward Timer | 実際のフォワードディレイタイマー
Msg Age Timer | ポートがBPDUの情報を破棄するタイマー。初期設定の場合、STPは20秒から、RSTP/MSTPは Hello Time×3の時間をカウントダウンする
Hello Timer | ハローを送信に使用するtimer。0になった時点でハローパケットを送信する
topo change timer | トポロジーチェンジタイマー
forward-transitions | ポートがForward Stateになった回数
Version | スパニングツリープロトコルの動作モード（バージョン）
Received | 受信した BPDU のタイプ
Send | 送信する BPDU のタイプ
portfast configured | エッジポートの設定値と現在の状態。portfast off、portfast on、edgeport onのいずれか
portfast bpdu-guard | インターフェースのBPDUガード機能の設定値と現在の状態
portfast bpdu-filter | インターフェースのBPDUフィルター機能の設定値と現在の状態
root guard configured | ルートガード機能の設定値と現在の状態
Configured Link Type | ポートのリンクタイプの設定値と現在の状態。point-to-point またはshared

### 注意・補足事項

■ MSTPモードのときは、CIST（インスタンス0）の情報が表示される。
■ 本コマンドはEXECモードだけでなくインターフェースモードでも実行できる。

### 関連コマンド

show spanning-tree mst（非特権EXECモード）

(C) 2018 - 2025 アライドテレシスホールディングス株式会社

PN: 613-002656 Rev.AL