[index] CentreCOM x320シリーズ コマンドリファレンス 5.5.5

# show ip prefix-list

モード: 非特権EXECモード
カテゴリー: IP / 経路制御（フィルタリング）

`> show ip prefix-list PLISTNAME`

`> show ip prefix-list [detail|summary] [PLISTNAME]`

IPプレフィックスリストを表示する。

### パラメーター

`PLISTNAME` | IPプレフィックスリスト名
`detail` | 詳細情報を表示させたいときに指定する
`summary` | サマリー情報を表示させたいときに指定する

### 使用例

■ オプション無指定時

    awplus> show ip prefix-list ↓
    ip prefix-list pDeny1620: 2 entries
         seq 5 deny 172.16.20.0/24
         seq 10 permit any
    ip prefix-list pDenyTen: 2 entries
       Description: Discard 10.0.0.0/8 prefixes.
         seq 5 deny 10.0.0.0/8 le 32
         seq 10 permit any

■ summaryオプション指定時

    awplus> show ip prefix-list summary ↓
    Prefix-list with the last deletion/insertion: pDeny1620
    ip prefix-list pDeny1620:
       count: 2, range entries: 0, sequences: 5 - 10
    ip prefix-list pDenyTen:
       Description: Discard 10.0.0.0/8 prefixes.
       count: 2, range entries: 0, sequences: 5 - 10

■ detailオプション指定時

    awplus> show ip prefix-list detail ↓
    Prefix-list with the last deletion/insertion: pDeny1620
    ip prefix-list pDeny1620:
       count: 2, range entries: 0, sequences: 5 - 10
        ripd:
         seq 5 deny 172.16.20.0/24 (hit count: 10, refcount: 20)
         seq 10 permit any (hit count: 10, refcount: 10)
        ospfd:
         seq 5 deny 172.16.20.0/24 (hit count: 0, refcount: 0)
         seq 10 permit any (hit count: 0, refcount: 0)
    ip prefix-list pDenyTen:
       Description: Discard 10.0.0.0/8 prefixes.
       count: 2, range entries: 0, sequences: 5 - 10
        ripd:
         seq 5 deny 10.0.0.0/8 le 32 (hit count: 28, refcount: 140)
         seq 10 permit any (hit count: 168, refcount: 168)
        ospfd:
         seq 5 deny 10.0.0.0/8 le 32 (hit count: 0, refcount: 0)
         seq 10 permit any (hit count: 0, refcount: 0)

### 関連コマンド

clear ip prefix-list（特権EXECモード）
ip prefix-list（グローバルコンフィグモード）

(C) 2020 - 2025 アライドテレシスホールディングス株式会社

PN: 613-002827 Rev.AB