[index] CentreCOM Secure HUB GS970EMXシリーズ コマンドリファレンス 5.5.5

# show spanning-tree statistics

モード: 特権EXECモード
カテゴリー: L2スイッチング / スパニングツリープロトコル

`# show spanning-tree statistics`

スパニングツリープロトコルのパラメーターや統計、タイマーなどの情報を表示する。

### 使用例

    awplus# show spanning-tree statistics ↓

                    Port number = 905 Interface = port1.0.1
                    ================================
    % BPDU Related Parameters
    % -----------------------
    % Port Spanning Tree                 : Enable
    % Spanning Tree Type                 : Rapid Spanning Tree Protocol
    % Current Port State                 : Forwarding
    % Port ID                            : 8389
    % Port Number                        : 389
    % Path Cost                          : 20000
    % Message Age                        : 0
    % Designated Root                    : 00:00:cd:28:06:b4
    % Designated Cost                    : 0
    % Designated Bridge                  : 00:00:cd:28:06:b4
    % Designated Port Id                 : 8389
    % Top Change Ack                     : FALSE
    % Config Pending                     : FALSE

    % PORT Based Information & Statistics
    % -----------------------------------
    % Config Bpdu's xmitted              : 443
    % Config Bpdu's received             : 2
    % TCN Bpdu's xmitted                 : 3
    % TCN Bpdu's received                : 0
    % Forward Trans Count                : 2

    % STATUS of Port Timers
    % ---------------------
    % Hello Time Configured              : 2
    % Hello timer                        : ACTIVE
    % Hello Time Value                   : 0
    % Forward Delay Timer                : INACTIVE
    % Forward Delay Timer Value          : 0
    % Message Age Timer                  : INACTIVE
    % Message Age Timer Value            : 0
    % Topology Change Timer              : INACTIVE
    % Topology Change Timer Value        : 0
    % Hold Timer                         : INACTIVE
    % Hold Timer Value                   : 0

    % Other Port-Specific Info
      ------------------------
    % Max Age Transitions                : 1
    % Msg Age Expiry                     : 0
    % Similar BPDUS Rcvd                 : 0
    % Src Mac Count                      : 1
    % Total Src Mac Rcvd                 : 2
    % Next State                         : Discard/Blocking
    % Topology Change Time               : 0

### 関連コマンド

show spanning-tree（非特権EXECモード）

(C) 2021 - 2025 アライドテレシスホールディングス株式会社

PN: 613-003033 Rev.T