[index] CentreCOM x240シリーズ コマンドリファレンス 5.5.5

# show atmf links statistics

モード: 特権EXECモード
カテゴリー: AMF / コマンド

`# show atmf links statistics [interface [IFRANGE]]`

対象ノードにおけるAMFの統計情報、または、対象ノードに設定されているAMF接続ポート（AMFリンク、AMFクロスリンク、AMFエリアリンク、AMFゲストリンク、AMFエージェントリンク、AMF仮想リンク）の統計情報を表示する。

### パラメーター

`interface [IFRANGE]` | 指定したインターフェースの統計情報を表示する。全体を省略した場合はノード全体としての統計が表示される。また、interfaceだけ指定してIFRANGEを省略した場合はすべてのAMF接続ポートの情報が表示される

### 使用例

■ AMFの統計情報（ノード全体）を表示する。

    SBx81# show atmf links statistics  ↓

     ATMF Statistics:

                                        Receive        Transmit
     --------------------------------------------------------------------------------
     Arealink Hello                       0              0
     Crosslink Hello                      0              0
     Crosslink Hello Domain               0              0
     Crosslink Hello Uplink               0              0
     Hello Link                           41             36
     Hello Neighbor                       57             58
     Hello Stack                          0              0
     Hello Gateway                        0              0
     Database Description                 21             26
     Database Request                     3              6
     Database Update                      27             28
     Database Update Bitmap               0              6
     Database Acknowledge                 20             21
     Transmit Fails                       0              0
     Discards                             0              0
     Total ATMF Packets                   169            181

     ATMF Database Statistics:

     Database Entries                     99
     Database Full Ages                   0

     ATMF Virtual Link Statistics:

     Virtual                              Receive                     Transmit
     link                   Receive       Dropped      Transmit       Dropped
     --------------------------------------------------------------------------------
     vlink1                      77             0            88             0
     vlink2                      70             0            83             0

     ATMF Packet Discards:

     Type0   0            : Gateway hello msg received from unexpected neighbor
     Type1   0            : Stack hello msg received from unexpected neighbor
     Type2   0            : Discard TX update bitmap packet - bad checksum
     Type3   0            : Discard TX update packet - neighbor not in correct state
     Type4   0            : Discard update packet - bad checksum or type
     Type5   0            : Discard update packet - neighbor not in correct state
     Type6   0            : Discard update bitmap packet - bad checksum or type
     Type7   0            : Incarnation is not possible with the data received
     Type8   0            : Discard crosslink hello received - not correct state
     Type9   0            : Discard crosslink domain hello received on non crosslink
     Type10  0            : Discard crosslink domain hello - not in correct state
     Type11  0            : Crosslink uplink hello received on non crosslink port
     Type12  0            : Discard crosslink uplink hello - not in correct state
     Type13  0            : Wrong network-name for this ATMF
     Type14  0            : Packet received on port is too long
     Type15  0            : Bad protocol version, received on port
     Type16  0            : Bad packet checksum calculation
     Type17  0            : Bad authentication type
     Type18  0            : Bad simple password
     Type19  0            : Unsupported authentication type
     Type20  0            : Discard packet - unknown neighbor
     Type21  0            : Discard packet - port is shutdown
     Type22  0            : Non broadcast hello msg received from unexpected neighbor
     Type23  0            : Arealink hello msg received on non arealink port
     Type24  0            : Discard arealink hello packet - not in correct state
     Type25  0            : Discard arealink hello packet - failed basic processing
     Type26  0            : Discard unicast packet - MAC address does not match node
     Type27  0            : AMF Master license node limit exceeded

■ AMF接続ポート（port1.1.1）の統計情報を表示する。

    SBx81# show atmf links statistics interface port1.1.1 ↓

     ATMF Port Statistics:

                                                  Receive        Transmit
     --------------------------------------------------------------------
     port1.1.1  Crosslink Hello                      0              0
     port1.1.1  Crosslink Hello Domain               0              0
     port1.1.1  Crosslink Hello Uplink               0              0
     port1.1.1  Hello Link                           20             19
     port1.1.1  Arealink Hello                       0              0

表 1
Receive | AMFパケット受信数（メッセージタイプごとに表示）
Transmit | AMFパケット送信数（メッセージタイプごとに表示）
Database Entries | AMFデータベースに存在するエントリーの数
Database Full Ages | AMFデータベース内でエントリーがエージアウトした回数
ATMF Packet Discards | AMFパケットを破棄した回数（破棄した理由ごとに表示）

表 2：AMFパケットの破棄理由一覧
Type 0 | 非クロスリンクポートでCrosslink Helloを受信したため破棄
Type 1 | チェックサム不正によりDatabase Updateを送信せずに破棄
Type 2 | チェックサム不正によりDatabase Update Bitmapを送信せずに破棄
Type 3 | 隣接ノードの状態不正によりDatabase Updateを送信せずに破棄
Type 4 | チェックサム不正によりDatabase Updateを破棄
Type 5 | 隣接ノードの状態不正によりDatabase Updateを破棄
Type 6 | チェックサム不正によりDatabase Update Bitmapを破棄
Type 7 | 非クロスリンクポートでCrosslink Helloを受信したため破棄
Type 8 | 受信ポートの状態不正によりCrosslink Helloを破棄
Type 9 | 非クロスリンクポートでCrosslink Domain Helloを受信したため破棄
Type 10 | 受信ポートの状態不正によりCrosslink Domain Helloを破棄
Type 11 | 非クロスリンクポートでCrosslink Uplink Helloを受信したため破棄
Type 12 | 受信ポートの状態不正によりCrosslink Uplink Helloを無視
Type 13 | AMFネットワーク名の不正により破棄
Type 14 | 受信パケットが長すぎるため破棄
Type 15 | 受信パケットのプロトコルバージョンが不正なため破棄
Type 16 | 受信パケットのチェックサムが不正なため破棄
Type 17 | 受信パケットの認証タイプが不正なため破棄
Type 18 | 受信パケットのパスワードが不正なため破棄
Type 19 | 受信パケットの認証タイプが未サポートなため破棄
Type 20 | 未知の隣接ノードから受信したパケットのため破棄
Type 21 | ポートがダウンしたため破棄
Type 22 | 意図しない隣接ノードからNon broadcast helloを受信したため破棄
Type 23 | 非エリアリンクポートでArealink helloを受信したため破棄
Type 24 | 状態不正によりArealink helloを破棄
Type 25 | 基本処理の失敗によりArealink helloを破棄
Type 26 | MACアドレスがノードと一致しないため、ユニキャストパケットを破棄
Type 27 | AMF/AMF Plusマスターライセンスのノード制限を超えたため破棄

### 関連コマンド

atmf virtual-link（グローバルコンフィグモード）
clear atmf links statistics（特権EXECモード）
show atmf links（特権EXECモード）
switchport atmf-crosslink（インターフェースモード）
switchport atmf-link（インターフェースモード）

(C) 2023 - 2025 アライドテレシスホールディングス株式会社

PN: 613-003248 Rev.N