[index] CentreCOM x240シリーズ コマンドリファレンス 5.5.5

# show auth

モード: 特権EXECモード
カテゴリー: インターフェース / ポート認証

`# show auth [interface [IFRANGE]|all]`

ポート認証の全般的情報、および、スイッチポートごとの情報を表示する。
オプションを指定せずに実行した場合は、全般的情報だけが表示される。
interfaceパラメーターを指定した場合は、インターフェースごとの情報だけが表示される。
allオプションを指定した場合は、全般的設定とすべてのインターフェースの情報が表示される。

### パラメーター

`interface [IFRANGE]` | スイッチポートごとの情報を表示する。特定ポートの情報だけを表示させたいときは、IFRANGEにスイッチポートのインターフェース名を指定する。ハイフン、カンマを使った複数指定も可能。省略時はポート認証の設定が行われているすべてのインターフェースが対象になる
`all` | システム全体の情報に加え、スイッチポートごとの情報も表示させたいときに指定する

### 使用例

    awplus# show auth ↓
    802.1X Port-Based Authentication Enabled
    MAC-based Port Authentication Enabled (Mode:Static)
    WEB-based Port Authentication Enabled
      RADIUS server address (auth): 172.16.10.186:1812
        Last radius message id: 10
      RADIUS server address (acct): 172.16.10.186:1813
        Last radius message id: 1

    awplus# show auth all ↓
    802.1X Port-Based Authentication Enabled
    MAC-based Port Authentication Enabled (Mode:Static)
    WEB-based Port Authentication Enabled
      RADIUS server address (auth): 172.16.10.186:1812
        Last radius message id: 10
      RADIUS server address (acct): 172.16.10.186:1813
        Last radius message id: 1
    Authentication Info for interface port1.0.1
      portEnabled: true - portControl: Auto
      portStatus: Authorized
      reAuthenticate: disabled
      reAuthPeriod: 3600
      PAE: quietPeriod: 60 - maxReauthReq: 2 - txPeriod: 30
      PAE: connectTimeout: 30
      BE: suppTimeout: 30 - serverTimeout: 30 - maxReq: 2
      CD: adminControlledDirections: in
      KT: keyTxEnabled: false
      critical: disabled
      guestVlan: disabled
      authFailVlan: disabled
      dynamicVlanCreation: disabled
      multiVlanSession: disabled
      hostMode: single-host
      dot1x: disabled
      authMac: enabled
        method: PAP
        reauthRelearning: disabled
      authWeb: disabled
      twoStepAuthentication:
        configured: disabled
        actual: disabled
      supplicantMac: none
      Supplicant name: 00-13-3b-0c-6c-2b
      Supplicant address: 0013.3b0c.6c2b
        authenticationMethod: MAC-based Authentication
        portStatus: Authorized - currentId: 1
        abort:F fail:F start:F timeout:F success:T
        PAE: state: Authenticated - portMode: Auto
        PAE: reAuthCount: 0 - rxRespId: 0
        PAE: quietPeriod: 60 - maxReauthReq: 2
        BE: state: Idle - reqCount: 0 - idFromServer: 0
        CD: adminControlledDirections: in - operControlledDirections: in
        CD: bridgeDetected: false
        KR: rxKey: false
        KT: keyAvailable: false - keyTxEnabled: false
        RADIUS server group (auth): radius
        RADIUS server (auth): 192.168.1.5

    awplus# show auth interface port1.0.1 ↓
    Authentication Info for interface port1.0.1
      portEnabled: true - portControl: Auto
      portStatus: Authorized
      reAuthenticate: disabled
      reAuthPeriod: 3600
      PAE: quietPeriod: 60 - maxReauthReq: 2 - txPeriod: 30
      PAE: connectTimeout: 30
      BE: suppTimeout: 30 - serverTimeout: 30 - maxReq: 2
      CD: adminControlledDirections: in
      KT: keyTxEnabled: false
      critical: disabled
      guestVlan: disabled
      authFailVlan: disabled
      dynamicVlanCreation: disabled
      multiVlanSession: disabled
      hostMode: single-host
      dot1x: disabled
      authMac: enabled
        method: PAP
        reauthRelearning: disabled
      authWeb: disabled
      twoStepAuthentication:
        configured: disabled
        actual: disabled
      supplicantMac: none

### 関連コマンド

aaa accounting auth-mac（グローバルコンフィグモード）
aaa authentication auth-mac（グローバルコンフィグモード）
auth multi-vlan-session（インターフェースモード）
auth two-step enable（インターフェースモード）
auth two-step order（インターフェースモード）
auth-mac enable（インターフェースモード）
auth-mac static（グローバルコンフィグモード）
auth-web enable（インターフェースモード）
show dot1x（特権EXECモード）

(C) 2023 - 2025 アライドテレシスホールディングス株式会社

PN: 613-003248 Rev.N