# redistribute

モード
  BGPモード
カテゴリー
  IP / 経路制御（BGP）

## 構文

コマンド構文

`(config-router)# [no] redistribute {connected|static|rip|ospf} [route-map NAME]`

## コマンド説明

指定した種類の非BGP経路をBGP経路表に追加する。これは、非BGP経路をBGPで再通知するための設定。
no形式でオプションを指定しなかった場合は、指定した種類の非BGP経路をBGP経路表から削除する。
no形式でオプションを指定した場合は、該当オプションをオフにする。

## パラメーター

`connected`
  インターフェース経路（直結経路）
`static`
  スタティック経路（ip routeコマンドで登録した経路）
`rip`
  RIP経路。RIPインターフェースの直結経路は含まれないので注意
`ospf`
  OSPF経路。OSPFインターフェースの直結経路は含まれないので注意
`route-map NAME`
  ルートマップ名。特定の非BGP経路だけを再通知したい場、あるいは再通知したくない場合、また、再通知する経路の属性を任意に設定したい場合などに指定する

## 使用例

    awplus(config)# do show ip bgp

    awplus(config)# do show ip route
    Codes: C - connected, S - static, R - RIP, B - BGP
           O - OSPF, IA - OSPF inter area
           N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
           E1 - OSPF external type 1, E2 - OSPF external type 2
           * - candidate default

    C       10.10.10.0/24 is directly connected, vlan1000
    C       172.16.10.0/24 is directly connected, vlan10
    C       172.16.20.0/24 is directly connected, vlan20
    C       172.16.30.0/24 is directly connected, vlan30
    C       172.16.40.0/24 is directly connected, vlan40
    C       172.16.50.0/24 is directly connected, vlan50
    C       172.16.60.0/24 is directly connected, vlan60
    C       172.16.70.0/24 is directly connected, vlan70
    C       172.16.80.0/24 is directly connected, vlan80
    C       172.16.90.0/24 is directly connected, vlan90

    awplus(config)# router bgp 65010
    awplus(config-router)# redistribute connected
    awplus(config-router)# do show ip bgp
    BGP table version is 48, local router ID is 10.10.10.1
    Status codes: s suppressed, d damped, h history, * valid, > best, i - internal,
                  S Stale
    Origin codes: i - IGP, e - EGP, ? - incomplete

       Network          Next Hop            Metric LocPrf Weight Path
    *> 10.10.10.0/24    0.0.0.0                            32768 ?
    *> 172.16.10.0/24   0.0.0.0                            32768 ?
    *> 172.16.20.0/24   0.0.0.0                            32768 ?
    *> 172.16.30.0/24   0.0.0.0                            32768 ?
    *> 172.16.40.0/24   0.0.0.0                            32768 ?
    *> 172.16.50.0/24   0.0.0.0                            32768 ?
    *> 172.16.60.0/24   0.0.0.0                            32768 ?
    *> 172.16.70.0/24   0.0.0.0                            32768 ?
    *> 172.16.80.0/24   0.0.0.0                            32768 ?
    *> 172.16.90.0/24   0.0.0.0                            32768 ?

    Total number of prefixes 10
    Total number of routes 10 (feature license allows maximum of 1000000)

## コマンドツリー

## 関連コマンド