[index] AT-ARX200S-GTX/AT-ARX200S-GT コマンドリファレンス 5.5.5

# show ip mroute

モード: 非特権EXECモード
カテゴリー: IPマルチキャスト / 一般設定

`> show ip mroute [ADDRESSES] [count|summary]`

IPマルチキャスト経路表（マルチキャスト配送ツリーの情報）を表示する。

### パラメーター

`ADDRESSES` | IPアドレス。次のいずれかの形式で指定する。指定時は指定したアドレスと合致するエントリーだけを表示する。省略時はすべてのエントリーを表示する
| `GROUP :=` | `A.B.C.D`
|  | マルチキャストグループアドレス
| `SOURCE :=` | `A.B.C.D`
|  | マルチキャスト送信者のIPアドレス
| `GROUP SOURCE :=` | `A.B.C.D A.B.C.D`
|  | マルチキャストグループアドレスとマルチキャスト送信者のIPアドレス
| `SOURCE GROUP :=` | `A.B.C.D A.B.C.D`
|  | マルチキャスト送信者のIPアドレスとマルチキャストグループアドレス
`count|summary` | 統計情報を表示（count）するかサマリー情報を表示（summary）するかを選択する。省略時は各エントリーの内容を表示する

### 使用例

    awplus> show ip mroute ↓

    IP Multicast Routing Table
    Flags: I - Immediate Stat, T - Timed Stat, F - Forwarder installed
    Timers: Uptime/Stat Expiry
    Interface State: Interface (TTL)

    (192.168.10.2, 239.1.2.3), uptime 00:01:41, stat expires 00:02:22
    Owner PIM-SM, Flags: TF
      Incoming interface: vlan10
      Outgoing interface list:
        Register (1)
        vlan30 (1)
        vlan20 (1)

    (192.168.20.2, 239.100.100.100), uptime 00:00:38, stat expires 00:03:22
    Owner PIM-SM, Flags: TF
      Incoming interface: vlan20
      Outgoing interface list:
        vlan30 (1)

    awplus> show ip mroute count ↓

    IP Multicast Statistics
    Total 2 routes using 272 bytes memory
    Route limit/Route threshold: 2048/2048
    Total NOCACHE/WRONGVIF/WHOLEPKT recv from fwd: 3/1/2
    Total NOCACHE/WRONGVIF/WHOLEPKT sent to clients: 3/1/2
    Immediate/Timed stat updates sent to clients: 0/0
    Reg ACK recv/Reg NACK recv/Reg pkt sent: 2/0/2
    Next stats poll: 00:00:16

    Forwarding Counts: Pkt count/Byte count, Other Counts: Wrong If pkts
    Fwd msg counts: WRONGVIF/WHOLEPKT recv
    Client msg counts: WRONGVIF/WHOLEPKT/Imm Stat/Timed Stat sent
    Reg pkt counts: Reg ACK recv/Reg NACK recv/Reg pkt sent

    (192.168.10.2, 239.1.2.3), Forwarding: 2/1, Other: 0
      Fwd msg: 1/1, Client msg: 1/1/0/0,  Reg: 1/0/1

    (192.168.20.2, 239.100.100.100), Forwarding: 1/0, Other: 0
      Fwd msg: 0/0, Client msg: 0/0/0/0,  Reg: 0/0/0

    awplus> show ip mroute summary ↓

    IP Multicast Routing Table
    Flags: I - Immediate Stat, T - Timed Stat, F - Forwarder installed
    Timers: Uptime/Stat Expiry
    Interface State: Interface (TTL)

    (192.168.10.2, 239.1.2.3), 00:02:14/00:03:29, PIM-SM, Flags: TF

    (192.168.20.2, 239.100.100.100), 00:01:11/00:03:29, PIM-SM, Flags: TF

### 関連コマンド

clear ip mroute statistics（特権EXECモード）

(C) 2024 - 2025 アライドテレシスホールディングス株式会社

PN: 613-003319 Rev.G