[index] SwitchBlade x908 GEN3 コマンドリファレンス 5.5.5

# show system environment

モード: 非特権EXECモード
カテゴリー: 運用・管理 / システム

`> show system environment`

本体、拡張モジュール、電源ユニット/ファンモジュールの動作環境に関する情報を表示する。

### 使用例

    awplus> show system environment ↓
    Environment Monitoring Status

    Stack member 1:

    Overall Status: Normal

    Resource ID: 9  Name: PSU Bay A ()
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                           No        -          -       Ok
    2   Fault                                    No        -          -       Ok
    3   PSU Power Output                         No        -          -       Ok
    4   PSU Power Input                          No        -          -       Ok

    Resource ID: 10  Name: PSU Bay B (AT-SBxPWRSYS2/AC)
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                          Yes        -          -       Ok
    2   Fault                                    No        -          -       Ok
    3   PSU Power Output                        Yes        -          -       Ok
    4   PSU Power Input                         Yes        -          -       Ok

    Resource ID: 11  Name: Fan Tray A (AT-FAN08)
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                          Yes        -          -       Ok

    Resource ID: 12  Name: Fan Tray B (AT-FAN08)
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                          Yes        -          -       Ok

    Resource ID: 100  Name: AT-SBx908 GEN3
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Temp: CPU (Degrees C)                    39        -           95     Ok
    2   Fan: Fan Tray A 1 Int (Rpm)            6122       3000        -       Ok
    3   Fan: Fan Tray A 1 Ext (Rpm)            5510       3000        -       Ok
    4   Fan: Fan Tray A 2 Int (Rpm)            6136       3000        -       Ok
    5   Fan: Fan Tray A 2 Ext (Rpm)            5465       3000        -       Ok
    6   Voltage: 0.8V (Volts)                 0.789      0.721      0.879     Ok
    7   Voltage: 0.88V (Volts)                0.868      0.791      0.967     Ok
    8   Voltage: 3.3V (Volts)                 3.317      2.960      3.631     Ok
    9   Voltage: 1.8V (Volts)                 1.791      1.617      1.978     Ok
    10  Voltage: 12V (Volts)                 12.012     10.767     13.166     Ok
    11  Temp: Remote 1 (Degrees C)               39        -11         81     Ok
    12  Temp: System (Degrees C)                 36        -11         73     Ok
    13  Temp: Remote 2 (Degrees C)               39        -11         84     Ok
    14  Fan: Fan Tray B 1 Int (Rpm)            6053       3000        -       Ok
    15  Fan: Fan Tray B 1 Ext (Rpm)            5567       3000        -       Ok
    16  Fan: Fan Tray B 2 Int (Rpm)            6136       3000        -       Ok
    17  Fan: Fan Tray B 2 Ext (Rpm)            5561       3000        -       Ok
    18  Voltage: 0.9V (Volts)                 0.899      0.809      0.984     Ok
    19  Voltage: 1.0V (Volts)                 0.995      0.896      1.099     Ok
    20  Voltage: 3.3V (Volts)                 3.325      2.960      3.631     Ok
    21  Voltage: 1.1V (Volts)                 1.105      0.993      1.195     Ok
    22  Voltage: 0.9V (Volts)                 0.938      0.800      0.984     Ok
    23  Temp: Remote 1 (Degrees C)               39        -11         78     Ok
    24  Temp: System (Degrees C)                 37        -11         76     Ok
    25  Temp: Remote 2 (Degrees C)               38        -11         78     Ok
    26  Temp: Chassis left (Degrees C)           36        -           66     Ok
    27  Temp: Chassis mid (Degrees C)            33        -           72     Ok
    28  Temp: Chassis right (Degrees C)          31        -           66     Ok
    29  Temp: Console (Degrees C)                35        -           62     Ok

    Resource ID: 101  Name: AT-XEM3-8CQ  Bay: 1
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Temp: XEM Front (Degrees C)              35    4(Hyst)         71     Ok
    2   Temp: XEM Rear (Degrees C)               42    4(Hyst)         78     Ok

    Resource ID: 102  Name: AT-XEM3-12XTm  Bay: 2
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Temp: XEM Front (Degrees C)              37    4(Hyst)         71     Ok
    2   Temp: XEM Rear (Degrees C)               41    4(Hyst)         78     Ok

    Resource ID: 103  Name: AT-XEM3-12YS  Bay: 3
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Temp: XEM Front (Degrees C)              30    4(Hyst)         71     Ok
    2   Temp: XEM Rear (Degrees C)               36    4(Hyst)         78     Ok

    ...

> Note

> > 上記表示は一例です。表示される内容は製品、バージョン、機器構成などによって異なります。

### 注意・補足事項

■ VCSマスターに対して本コマンドを実行した場合は、すべてのスタックメンバーに関する情報を表示する。

### 関連コマンド

show system（非特権EXECモード）
show system pluggable（非特権EXECモード）

(C) 2025 アライドテレシスホールディングス株式会社

PN: 613-003380 Rev.C