[index] AT-TQ6702e GEN2-R コマンドリファレンス 5.5.5

# show wireless network(local)

モード: 非特権EXECモード
カテゴリー: 無線機能 / 無線ネットワーク設定

`> show wireless network [<1-65535>|all] [brief]`

無線ネットワークの設定内容を表示する。

### パラメーター

`<1-65535>` | 無線ネットワーク設定番号。カンマ、ハイフン区切りで複数指定が可能。本パラメーター指定時は指定したネットワークだけを表示する。省略時はallを指定したのと同じ動作となる
`all` | すべてのネットワークを表示する（省略時動作）
`brief` | 無線ネットワークの情報を簡潔に表示させたいときに指定する。省略時は詳細な情報が表示される

### 使用例

    awplus> show wireless network 1 ↓
    Network ID 1:
     Description ...................
     Assigned VLAN ID .............. 1
     SSID .......................... allied24
     Hide SSID ..................... -
     Band-Steering ................. Disable
     Association Advertisement ..... Disable
     Duplicate AUTH Received ....... Disconnect
     DTIM Period ................... 1
     Proxy ARP ..................... Disable
     BSS Transition Management ..... Disable
     Security ID ................... -
      Security Mode ................ -
     MAC-Auth
      Authentication Mode .......... radius
      RADIUS group .................
      Username
       Separator ................... hyphen
       Character Case .............. lower-case
      Password .....................
      RADIUS Send Service Type ..... Disable
      RADIUS DAS IP Address ........
      Dynamic VLAN ................. Disable
      Critical Mode ................ Disable
     RADIUS group for Web-Auth .....
     Wireless MAC filter ID ........ 1
     Inactivity Timer .............. 300
     Client Isolation Mode ......... Disabled
     Unassociated Client List ...... Not acquire
     Airtime Fairness Percentage.... 0
     Multicast Unicast Conversion .. Disable
    Captive-Portal ................. Disable
      Authentication Mode .......... click-through
      RADIUS group .................
      RADIUS Accounting  ........... Disable
      External Page URL ............
      Redirect URL .................
      Session keep ................. Disable
      Session Timeout Interval ..... 3600
      Session Timeout Action . ..... Reauthentication
      Page proxy URL ...............
      Walled Garden Entries ........ 0
      DNS Proxy for Walled Garden .. Disable
    Passpoint ..................... Enable
      802.11u
       Access Network Type ......... private
       Internet Access ............. Enable
       Additional Step Required .... Disable
       ES Reacheable ............... Disable
       Venue Group ................. 7
       Venue Type .................. 1
       Unauth ES accessible ........ Disable
       Homogeneous ESSID ...........
       Roaming Consortium List .....
       Venue Name Information ......
       Network Auth Type ...........
       IP Type Availability v4/v6 .. port-private-nat1/no-exist
       Domain Name .................
       3GPP Info (MCC,MNC) .........
       NAI Realm Information ......
       ANQP-element ...............
       GAS Address 3 Behavior ..... 0
       GAS Comeback Delay ......... 0
       QoS Map Set configuration ..
      Hotspot 2.0
       DGAF ........................ Enable
       L2 Traf Inspect and Filter .. Disable
       ANQP Domain ID .............. 0
       Deauth Request Timeout ...... 60
       Operator Friendly Name .....
       Connection Capability ......
       WAN Metrics
        WAN Information ............ 01
        Speed Uplink/Downlink ...... 1000/8000
        Load Uplink/Downlink ....... 240/80
        Load Measure Duration ...... 3000
       Operating Class Indication ..
    Network ID 17:
     Description ...................
     Assigned VLAN ID .............. 1
     SSID .......................... allied5
     Hide SSID ..................... -
     Band-Steering ................. Disable
     Association Advertisement ..... Disable
     Duplicate AUTH Received ....... Disconnect
     DTIM Period ................... 1
     Proxy ARP ..................... Disable
     BSS Transition Management ..... Disable
     Security ID ................... -
      Security Mode ................ -
     MAC-Auth
      Authentication Mode .......... radius
      RADIUS group .................
      Username
       Separator ................... hyphen
       Character Case .............. lower-case
      Password .....................
      RADIUS Send Service Type ..... Enable
      RADIUS DAS IP Address ........ 192.168.1.1
      Dynamic VLAN ................. Disable
      Critical Mode ................ Disable
     RADIUS group for Web-Auth .....
     Wireless MAC filter ID ........ 2
     Inactivity Timer .............. 300
     Client Isolation Mode ......... Disabled
     Unassociated Client List ...... Acquire
     Airtime Fairness Percentage.... 3
     Multicast Unicast Conversion .. Enable
     Captive-Portal ................ Disable
      Authentication Mode .......... click-through
      RADIUS group .................
      RADIUS Accounting  ........... Disable
      External Page URL ............
      Redirect URL .................
      Session keep ................. Disable
      Session Timeout Interval ..... 3600
      Session Timeout Action . ..... Reauthentication
      Page proxy URL ...............
      Walled Garden Entries ........ 0
      DNS Proxy for Walled Garden .. Disable
    Passpoint ..................... Enable
      802.11u
       Access Network Type ......... public
       Internet Access ............. Enable
       Additional Step Required .... Enable
       ES Reacheable ............... Enable
       Unauth ES Accessible ........ Enable
       Homogeneous ESSID ........... 1234.5678.9abc
       Roaming Consortium List ..... 021122,02233445566
       Network Auth Type
        Auth Type .................. redirect-http-https
        Redirect URL ............... http://www.example.com/redirect/me/here
       IP Type Availability v4/v6 .. public/no-exist
       Domain Name ................. example.com,google.com
       3GPP Info (MCC,MNC) ......... 244,91;310,261
       NAI Realm Information
        ID  1:
         Realm Name ................ example.com,example.net
         EAP Method ................ EAP-TLS
        ID  2:
         Realm Name ................ example.com;example.net
         EAP Method ................ EAP-TLS,EAP-TTLS/MSCHAPv2
       ANQP-element Configuration
        Info ID    1: Payload ...... 0000
        Info ID   20: Payload ...... 00000000
       GAS Address 3 Behavior ...... 0
       GAS Comeback Delay .......... 1000
       QoS Map Set configuration ... 53,2,22,6,8,15,0,7,255,255,16,31,32,39,255,255,40,47,255,255
      Hotspot2.0
       DGAF ........................ Disable
       L2 Traf Inspect and Filter .. Disable
       ANQP Domain ID .............. 0
       Deauth Request Timeout ...... 60
       Operator Friendly Name
        ID  1:
         Language Code ............. jpn
         Friendly Name ............. TestJP
        ID  2:
         Language Code ............. eng
         Friendly Name ............. TestNZ
       Connection Capability
         IP Protocol 1:
          Port ..................... 0
          Status ................... open
         IP Protocol 12:
          Port ..................... 80
          Status ................... open
       WAN Metrics
         WAN Information ........... 01
         Speed Uplink/Downlink ..... 384/2500
         Load Uplink/Downlink ...... 0/0
         Load Measure Duration ..... 10
       Operating Class Indication .. 51

    awplus> show wireless network brief ↓
    ID    VLAN SSID                             H Sec ID MAC-Auth Web-Auth
    ----- ---- -------------------------------- - ------ -------- --------
        1    1 allied24                         -      -        -        -
        2    1 Virtual Access Point1            -      -        -        -
       17    1 allied5                          -      -        -        -

### 関連コマンド

network(local)（無線設定モード）

(C) 2025 アライドテレシスホールディングス株式会社

PN: 613-003429 Rev.B