# show system environment

モード
  非特権EXECモード
カテゴリー
  運用・管理 / システム

## 構文

コマンド構文

`> show system environment`

## コマンド説明

製品の動作環境に関する情報（環境センサーの情報）を表示する。
表示される内容は製品、バージョン、機器構成などによって異なる。

## 使用例

    awplus> show system environment
    Environment Monitoring Status

    Card 1.1:

    Overall Status: Normal

    Resource ID: 100  Name: AT-SBx81XLEM
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Voltage: 1.8V (Volts)                 1.784      1.615      1.979     Ok
    2   Voltage: 1.5V (Volts)                 1.491      1.350      1.645     Ok
    3   Voltage: 3.3V (Volts)                 3.283      2.973      3.627     Ok
    4   Voltage: 3.3V (Volts)                 3.307      2.969      3.620     Ok
    5   Voltage: 12.0V (Volts)               12.250     10.813     13.188     Ok
    6   Voltage: 1.0V (Volts)                 1.027      0.900      1.097     Ok
    7   Temp: Middle (Degrees C)                 54   70(Hyst)         75     Ok
    8   Temp: Front (Degrees C)                  40   60(Hyst)         65     Ok

    Card 1.3:

    Overall Status: Normal

    Resource ID: 100  Name: AT-SBx81XLEM
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Voltage: 1.8V (Volts)                 1.797      1.615      1.979     Ok
    2   Voltage: 1.5V (Volts)                 1.491      1.350      1.645     Ok
    3   Voltage: 3.3V (Volts)                 3.283      2.973      3.627     Ok
    4   Voltage: 3.3V (Volts)                 3.307      2.969      3.620     Ok
    5   Voltage: 12.0V (Volts)               12.250     10.813     13.188     Ok
    6   Voltage: 1.0V (Volts)                 1.027      0.900      1.097     Ok
    7   Temp: Middle (Degrees C)                 54   70(Hyst)         75     Ok
    8   Temp: Front (Degrees C)                  41   60(Hyst)         65     Ok

    Card 1.5:

    Overall Status: Normal

    Resource ID: 13  Name: PSU Bay A ()
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                           No        -          -       Ok
    2   Fault                                    No        -          -       Ok
    3   PSU Power Output                         No        -          -       Ok
    4   PSU Power Input                          No        -          -       Ok

    Resource ID: 14  Name: PSU Bay B ()
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                           No        -          -       Ok
    2   Fault                                    No        -          -       Ok
    3   PSU Power Output                         No        -          -       Ok
    4   PSU Power Input                          No        -          -       Ok

    Resource ID: 15  Name: PSU Bay C (AT-SBxPWRSYS2/AC)
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                          Yes        -          -       Ok
    2   Fault                                    No        -          -       Ok
    3   PSU Power Output                        Yes        -          -       Ok
    4   PSU Power Input                         Yes        -          -       Ok

    Resource ID: 16  Name: PSU Bay D ()
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                           No        -          -       Ok
    2   Fault                                    No        -          -       Ok
    3   PSU Power Output                         No        -          -       Ok
    4   PSU Power Input                          No        -          -       Ok

    Resource ID: 17  Name: Fan Tray Slot (AT-SBxFAN12)
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                          Yes        -          -       Ok
    2   Fault                                    No        -          -       Ok

    Resource ID: 100  Name: AT-SBx81CFC960 v2
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Voltage: 2.5V (Volts)                 2.461      2.344      2.865     Ok
    2   Voltage: Battery (Volts)              3.094      2.700      3.586     Ok
    3   Voltage: 3.3V (Volts)                 3.300      2.973      3.627     Ok
    4   Voltage: 1.0V (Volts)                 0.998      0.900      1.097     Ok
    5   Temp: Internal (Degrees C)               53   65(Hyst)         70     Ok

    Resource ID: 117  Name: AT-SBxFAN12
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Fan: Fan 1 (Rpm)                       2955         82        -       Ok
    2   Fan: Fan 2 (Rpm)                       2968         82        -       Ok
    3   Fan: Fan 3 (Rpm)                       2944         82        -       Ok
    4   Fan: Fan 4 (Rpm)                       2970         82        -       Ok
    5   Temp: Temperature 1 (Degrees C)          32         -5         60     Ok
    6   Temp: Temperature 2 (Degrees C)          32         -5         60     Ok
    7   Temp: Temperature 3 (Degrees C)          30         -5         60     Ok

    Card 1.6:

    Overall Status: Normal

    Resource ID: 100  Name: AT-SBx81CFC960
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Voltage: 2.5V (Volts)                 2.487      2.344      2.865     Ok
    2   Voltage: Battery (Volts)              3.080      2.700      3.586     Ok
    3   Voltage: 3.3V (Volts)                 3.283      2.973      3.627     Ok
    4   Voltage: 1.0V (Volts)                 0.998      0.900      1.097     Ok
    5   Temp: Internal (Degrees C)               44   65(Hyst)         70     Ok

    ...

Note

上記表示は一例です。表示される内容は製品、バージョン、機器構成などによって異なります。

## 注意・補足事項

VCSマスターに対して本コマンドを実行した場合は、すべてのスタックメンバーに関する情報を表示する。
電源ユニットスロット（PSU 1、PSU 2）は、電源ユニットが装着されていない場合でもStatus「Ok」と表示される。

## 関連コマンド