# test interface

モード
  特権EXECモード
カテゴリー
  インターフェース / 一般設定

## 構文

コマンド構文

`# test interface {IFRANGE|all} [time {<1-60>|cont} | second <1-3600>] [fixed]`

`# no test interface {IFRANGE|all}`

## コマンド説明

指定したインターフェースに対してテストパケットの送信を開始する。
no形式で実行した場合はテストパケットの送信を停止する。

## パラメーター

`IFRANGE`
  ポートリスト。ハイフン、カンマを使った複数指定が可能
`all`
  すべてのポートを指定する
`time {<1-60>|cont}`
  テストの継続時間
  `<1-60>`
    継続時間（分）
  `cont`
    本コマンドをno形式で実行するまでテストを継続する
`second <1-3600>`
  テストの継続時間（秒）
`fixed`
  Specifies that the test module should run at fixed speed, rather than scanning through speed settings while running the traffic test.

## 使用例

To test the switch ports in VLAN 1, install loopbacks in the ports, and enter the following commands:

    awplus(config)# service test
    awplus(config)# no spanning-tree rstp enable bridge-forward
    awplus(config)# interface vlan1
    awplus(config-if)# shutdown
    awplus(config-if)# end
    awplus# test interface all

To see the output, use the commands:

    awplus# show test
    awplus# show test count

To start the test on all interfaces for 1 minute use the command:

    awplus# test interface all time 1

To start the test on ports 1 to 12 for XEM 1 (port1.1.1 through port1.1.12) use the command:

    awplus# test interface port1.1.1-port1.1.12

To stop testing ports 1 to 12 for XEM 1 (port1.1.1 through port1.1.12) use the command:

    awplus# no test interface port1.1.1-port1.1.12

To start the test on all interfaces for 1 minute at a fixed speed use the command:

    awplus# test interface all time 1 fixed

## 関連コマンド