# show etherchannel

モード
  非特権EXECモード
カテゴリー
  インターフェース / リンクアグリゲーション（IEEE 802.3ad）

## 構文

コマンド構文

`> show etherchannel [summary|detail|<1-32>]`

## コマンド説明

LACPチャンネルグループの情報を表示する。
オプションを指定しなかった場合は、定義済みLACPチャンネルグループの所属ポート一覧が表示される。
オプションを指定した場合は、LACPチャンネルグループの情報と所属ポートの情報が表示される。

## パラメーター

`summary`
  定義済みのすべてのLACPチャンネルグループの情報を簡潔に表示する
`detail`
  定義済みのすべてのLACPチャンネルグループの詳細情報を表示する
`<1-32>`
  LACPチャンネルグループ番号。指定したLACPチャンネルグループの詳細情報を表示する

## 使用例

    awplus> show etherchannel
    LAG Maximum        : XXX
    LAG Static  Maximum: XX
    LAG Dynamic Maximum: XX
    LAG Static  Count  : 0
    LAG Dynamic Count  : 1
    LAG Total   Count  : 1
    Lacp Aggregator: po1
    Member:
     port1.0.1
     port1.0.2
     port1.0.3
     port1.0.4

    awplus> show etherchannel summary
    Aggregator po1 (IfIndex: 4601)
     Admin Key: 0001 - Oper Key 0001
      Link: port1.0.1 (IfIndex: 5001) synchronized
      Link: port1.0.2 (IfIndex: 5002) synchronized
      Link: port1.0.3 (IfIndex: 5003) disabled
      Link: port1.0.4 (IfIndex: 5004) synchronized

    awplus> show etherchannel detail
    Aggregator po1 (IfIndex: 4601)
     Mac address: ec:cd:6d:9d:4e:d5
     Admin Key: 0001 - Oper Key 0001
     Receive link count: 3 - Transmit link count: 3
     Individual: 0 - Ready: 1
     Partner LAG: 0x8000,ec-cd-6d-a3-f8-ae,0x0001
      Link: port1.0.1 (IfIndex: 5001) synchronized
      Link: port1.0.2 (IfIndex: 5002) synchronized
      Link: port1.0.3 (IfIndex: 5003) disabled
      Link: port1.0.4 (IfIndex: 5004) synchronized

## 関連コマンド