# show atmf secure-mode sa

モード
  特権EXECモード
カテゴリー
  AMF / コマンド

## 構文

コマンド構文

`# show atmf secure-mode sa [detail] [TYPE]`

## コマンド説明

AMFセキュアモード（atmf secure-mode）におけるAMFノード間の信頼関係（SA）情報を表示する。
セキュアモード無効時はエラーとなる。

## パラメーター

`detail`
  詳細な情報を表示させたいときに指定する
`TYPE := [link & neighbor & broadcast]`
  表示する情報の種類。スペース区切りで複数指定可能。省略時はすべての情報が表示される
  `link`
    リンク情報
  `neighbor`
    ネイバー情報
  `broadcast`
    ブロードキャスト情報

## 使用例

通常表示。

    SBx81a# show atmf secure-mode sa

      ATMF Security Associations:

      Type                       State           ID            Details
    --------------------------------------------------------------------------------
      Neighbor Node              Complete        175           FSW242
      Broadcast                  Complete        4095
      CrossLink                  Complete        4501          sa1
      AreaLink                   Cert Exchg      4511          sa11
      Link                       Complete        6009          port1.2.9
      AreaLink                   CA Exchg Init   6013          port1.2.13
      AreaLink                   Cert Exchg      13001         port1.9.1
      Link                       CA Exchg Init   16779521      vlink3
      Neighbor Gateway           Complete        83            FSW241
      Neighbor Gateway           Complete        175           FSW242
      Neighbor Cntl-Master       Complete        83            FSW241
      Neighbor Cntl-Master       Complete        175           FSW242
      Neighbor Cntl-Master       Complete        321           FSW243

詳細表示。

    SBx81a# show atmf secure-mode sa detail

     Security Associations Detail:

    --------------------------------------------------------------------------------
    Id                      : 175 (af)
      Type                  : Neighbor Node
      State                 : Complete
      Remote MAC Address    : eccd.6d82.6c16
      Flags                 : 000003c0

    Id                      : 4095 (fff)
      Type                  : Broadcast
      State                 : Complete
      Originator Node ID    : 175
      Flags                 : 00000200

    Id                      : 4501 (1195)
      Type                  : CrossLink
      State                 : Complete
      Remote MAC Address    : eccd.6d82.6c16
      Flags                 : 000003c0

    Id                      : 4511 (119f)
      Type                  : AreaLink
      State                 : Cert Exchg
      Remote MAC Address    : 0000.cd37.0081
      Flags                 : 00000060

    Id                      : 6009 (1779)
      Type                  : Link
      State                 : Complete
      Remote MAC Address    : 001a.eb54.e53b
      Flags                 : 000003c0

    Id                      : 6013 (177d)
      Type                  : AreaLink
      State                 : Init
      Remote MAC Address    : 0000.0000.0000
      Flags                 : 00000000

    Id                      : 13001 (32c9)
      Type                  : AreaLink
      State                 : Cert Exchg
      Remote MAC Address    : 0000.cd37.0003
      Flags                 : 00000060

    Id                      : 16779521 (1000901)
      Type                  : Link
      State                 : CA Exchg Init
      Remote MAC Address    : 0000.0000.0000
      Flags                 : 00000001

    Id                      : 83 (40000053)
      Type                  : Neighbor Gateway
      State                 : Complete
      Remote MAC Address    : 001a.eb54.e53b
      Flags                 : 000003c0

    Id                      : 175 (400000af)
      Type                  : Neighbor Gateway
      State                 : Complete
      Remote MAC Address    : eccd.6d82.6c16
      Flags                 : 000003c0

    Id                      : 83 (80000053)
      Type                  : Neighbor Cntl-Master
      State                 : Complete
      Remote MAC Address    : 001a.eb54.e53b
      Flags                 : 000003c0

    Id                      : 175 (800000af)
      Type                  : Neighbor Cntl-Master
      State                 : Complete
      Remote MAC Address    : eccd.6d82.6c16
      Flags                 : 000003c0

    Id                      : 321 (80000141)
      Type                  : Neighbor Cntl-Master
      State                 : Complete
      Remote MAC Address    : 0000.f427.93da
      Flags                 : 000003c0