# show port-security intrusion

モード
  特権EXECモード
カテゴリー
  インターフェース / スイッチポート

## 構文

コマンド構文

`# show port-security intrusion [interface IFNAME]`

## コマンド説明

ポートセキュリティー機能が検出した不正MACアドレスの一覧を表示する。

## パラメーター

`interface IFNAME`
  スイッチポートのインターフェース名。省略時はすべてのスイッチポートが対象となる

## 使用例

    awplus# show port-security intrusion
    Port Security Intrusion List
    ------------------------------------------------------------
    Interface: port1.0.1    -   2 intrusion(s) detected
      00-0c-29-04-49-46  00-0a-79-34-06-12
    Interface: port1.0.2    -   no intrusions detected
    Interface: port1.0.3    -   no intrusions detected
    Interface: port1.0.4    -   no intrusions detected
    Interface: port1.0.5    -   no intrusions detected
    Interface: port1.0.6    -   no intrusions detected
    Interface: port1.0.7    -   no intrusions detected
    Interface: port1.0.8    -   no intrusions detected
    Interface: port1.0.9    -   no intrusions detected
    Interface: port1.0.10   -   no intrusions detected
    Interface: port1.0.11   -   no intrusions detected
    Interface: port1.0.12   -   no intrusions detected
    Interface: port1.0.13   -   no intrusions detected
    Interface: port1.0.14   -   no intrusions detected
    Interface: port1.0.15   -   no intrusions detected
    Interface: port1.0.16   -   no intrusions detected
    Interface: port1.0.17   -   no intrusions detected
    Interface: port1.0.18   -   no intrusions detected
    Interface: port1.0.19   -   no intrusions detected
    Interface: port1.0.20   -   no intrusions detected
    Interface: port1.0.21   -   no intrusions detected
    Interface: port1.0.22   -   no intrusions detected
    Interface: port1.0.23   -   no intrusions detected
    Interface: port1.0.24   -   no intrusions detected

## 関連コマンド