# show ipv6 pim sparse-mode mroute

モード
  非特権EXECモード
カテゴリー
  IPv6マルチキャスト / PIM

## 構文

コマンド構文

`> show ipv6 pim sparse-mode mroute [[ADDRESSES] [detail] | brief]`

## コマンド説明

（PIM-SMv6）PIM-SMv6経路表を表示する。

## パラメーター

`ADDRESSES`
  IPv6アドレス。次のいずれかの形式で指定する。指定時は指定したアドレスと合致するエントリーだけを表示する。省略時はすべてのエントリーを表示する
  `GROUP := X:X::X:X`
    マルチキャストグループアドレス
  `SOURCE := X:X::X:X`
    マルチキャスト送信者のIPv6アドレス
  `GROUP SOURCE := X:X::X:X X:X::X:X`
    マルチキャストグループアドレスとマルチキャスト送信者のIPv6アドレス
  `SOURCE GROUP := X:X::X:X X:X::X:X`
    マルチキャスト送信者のIPv6アドレスとマルチキャストグループアドレス
`detail`
  詳細な情報を表示する
`brief`
  PIM-SMv6経路表に関するサマリーを表示する

## 使用例

    awplus# show ipv6 pim sparse-mode mroute
    IPv6 Multicast Routing Table

    (*,*,RP) Entries: 0
    (*,G) Entries: 2
    (S,G) Entries: 0
    (S,G,rpt) Entries: 0
    FCR Entries: 2

    (*, ff0x::db8:0:0/96)
    RP: 2001:db8:10:5::153
    RPF nbr: fe80::202:b3ff:fed4:69fe
    RPF idx: wm0
    Upstream State: JOINED
     Local     1
     Joined    0
     Asserted  0
    FCR:
    Source: 2001:db8:10:1::96
     Outgoing  1
     KAT timer running, 205 seconds remaining
     Packet count 1

    (*, ff0x::db8:0:0/96)
    RP: 2001:db8:10:5::153
    RPF nbr: fe80::202:b3ff:fed4:69fe
    RPF idx: wm0
    Upstream State: JOINED
     Local     1
     Joined    0
     Asserted  0
    FCR:
    Source: 2001:db8:10:1::96
     Outgoing  1
     KAT timer running, 208 seconds remaining
     Packet count 1

    awplus# show ipv6 pim sparse-mode mroute detail
    IPv6 Multicast Routing Table

    (*,*,RP) Entries: 0
    (*,G) Entries: 1
    (S,G) Entries: 0
    (S,G,rpt) Entries: 0
    FCR Entries: 0

    (*, ff13::10) Uptime: 00:00:09
      RP: ::, RPF nbr: None, RPF idx: None
      Upstream:
       State: JOINED, SPT Switch: Enabled, JT: off
       Macro state: Join Desired,
      Downstream:
       vlan2:
         State: NO INFO, ET: off, PPT: off
         Assert State: NO INFO, AT: off
          Winner: ::, Metric: 4294967295l, Pref: 4294967295l, RPT bit: on
         Macro state: Could Assert, Assert Track
      Local Olist:
       vlan3
      FCR:

## 注意・補足事項

本機能の設定を行う際は、あらかじめPIM6サービスを有効にしておくこと（service pim6コマンド）。

## 関連コマンド