# show ipv6 ospf

モード
  非特権EXECモード
カテゴリー
  IPv6 / 経路制御（OSPFv3）

## 構文

コマンド構文

`> show ipv6 ospf [PROCID]`

## コマンド説明

OSPFv3ルーティングプロセスの情報を表示する。

## パラメーター

`PROCID`
  router ipv6 ospfコマンドで設定したOSPFv3ルーティングプロセスID。省略時は稼働中のすべてのプロセスが対象となる

## 使用例

    awplus> show ipv6 ospf
     Routing Process "OSPFv3 (*null*)" with ID 10.10.10.1
     Route Licence: Route : Limit=Unlimited, Allocated=7, Visible=6, Internal=1
     Route Licence: Breach: Current=0, Watermark=0
     Process uptime is 17 minutes
     Current grace period is 120 secs (default)
     SPF schedule delay min 0.500 secs, SPF schedule delay max 50.0 secs
     Minimum LSA interval 5 secs, Minimum LSA arrival 1 secs
     Number of incoming current DD exchange neighbors 0/5
     Number of outgoing current DD exchange neighbors 0/5
     Number of external LSA 1. Checksum Sum 0x3CA0
     Number of AS-Scoped Unknown LSA 0
     Number of LSA originated 15
     Number of LSA received 10
     Number of areas in this router is 2
        Area BACKBONE(0)
            Number of interfaces in this area is 1(1)
            SPF algorithm executed 7 times
            Number of LSA 8.  Checksum Sum 0x37047
            Number of Unknown LSA 0
        Area 1.1.1.1
            Number of interfaces in this area is 2(2)
            SPF algorithm executed 1 times
            Number of LSA 6.  Checksum Sum 0x37EA3
            Number of Unknown LSA 0

## 注意・補足事項

本機能の設定を行う際は、あらかじめOSPF6サービスを有効にしておくこと（service ospf6コマンド）。

## 関連コマンド