# show ipv6 mld snooping statistics interface

モード
  非特権EXECモード
カテゴリー
  IPv6マルチキャスト / MLD Snooping

## 構文

コマンド構文

`> show ipv6 mld [vrf VRFNAME|global] snooping statistics interface IFNAME`

## コマンド説明

MLD Snoopingが管理しているマルチキャストグループメンバーの情報を表示する。

## パラメーター

`vrf VRFNAME`
  VRFインスタンス名。指定したVRFインスタンスのみ表示するときに指定する
`global`
  グローバルVRFインスタンスのみ表示するときに指定
`IFNAME`
  VLANインターフェース名

## 使用例

    awplus> show ipv6 mld snooping statistics interface vlan1
    MLD Snooping statistics for vlan1
    Interface:      port1.1.1
    Group:          ff02::1:ff60:5a66
    Uptime:         00:07:13
    Group mode:     Exclude (Expires: 00:03:25)
    Last reporter:  fe80::20c:29ff:fe60:5a66
    Source list is empty

    Interface:      port1.1.1
    Group:          ff02::2:abcc:66f8
    Uptime:         00:07:13
    Group mode:     Exclude (Expires: 00:03:25)
    Last reporter:  fe80::20c:29ff:fe60:5a66
    Source list is empty

    Interface:      port1.1.1
    Group:          ff1e::ca:331
    Uptime:         00:03:25
    Group mode:     Exclude (Expires: 00:03:25)
    Last reporter:  fe80::20c:29ff:fe60:5a66
    Source list is empty

    Group Type:     Router Port Learnt
    Interface:      port1.1.8
    Group:          ff02::2
    Uptime:         00:09:50
    Group mode:     Exclude (Expires: 00:03:51)
    Last reporter:  fe80::200:f4ff:fe27:2c74

## 関連コマンド