# show ip rpf

モード
  非特権EXECモード
カテゴリー
  IPマルチキャスト / 一般設定

## 構文

コマンド構文

`> show ip rpf [vrf VRFNAME|global] A.B.C.D`

## コマンド説明

指定したIPマルチキャスト送信者アドレスへのRPF（Reverse Path Forwarding）情報を表示する。

## パラメーター

`vrf VRFNAME`
  VRFインスタンス名。指定したVRFインスタンスのみ表示するときに指定する
`global`
  グローバルVRFインスタンスのみ表示するときに指定
`A.B.C.D`
  マルチキャスト送信者のIPアドレス（S）

## 使用例

    awplus> show ip rpf 192.168.10.2
    RPF information for 192.168.10.2
      RPF interface: vlan10
      RPF neighbor: 0.0.0.0
      RPF route: 192.168.10.0/24
      RPF type: unicast (connected)
      RPF recursion count: 0
      Doing distance-preferred lookups across tables
      Distance: 0
      Metric: 0

    awplus> show ip rpf 192.168.40.2
    RPF information for 192.168.40.2
      RPF interface: vlan30
      RPF neighbor: 192.168.30.254
      RPF route: 192.168.40.0/24
      RPF type: unicast (rip)
      RPF recursion count: 0
      Doing distance-preferred lookups across tables
      Distance: 120
      Metric: 2

    awplus> show ip rpf 172.21.10.2
    RPF information for 172.21.10.2
      RPF interface: vlan30
      RPF neighbor: 172.18.10.2
      RPF route: 172.21.10.0/24
      RPF type: unicast (ospf)
      RPF recursion count: 0
      Doing distance-preferred lookups across tables
      Distance: 110
      Metric: 2
    awplus> show ip rpf 172.16.10.2
    RPF information for 172.16.10.2
      RPF interface: vlan10
      RPF neighbor: 0.0.0.0
      RPF route: 172.16.10.0/24
      RPF type: unicast (connected)
      RPF recursion count: 0
      Doing distance-preferred lookups across tables
      Distance: 0
      Metric: 0

## 関連コマンド