# show system environment

モード
  非特権EXECモード
カテゴリー
  運用・管理 / システム

## 構文

コマンド構文

`> show system environment`

## コマンド説明

製品の動作環境に関する情報（環境センサーの情報）を表示する。
表示される内容は製品、バージョン、機器構成などによって異なる。

## 使用例

    awplus> show system environment
    Environment Monitoring Status

    Stack member 1:

    Overall Status: Normal

    Resource ID: 9  Name: PSU Bay A ()
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                           No        -          -       Ok
    2   Fault                                    No        -          -       Ok
    3   PSU Power Output                         No        -          -       Ok
    4   PSU Power Input                          No        -          -       Ok

    Resource ID: 10  Name: PSU Bay B (AT-SBxPWRSYS2/AC)
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                          Yes        -          -       Ok
    2   Fault                                    No        -          -       Ok
    3   PSU Power Output                        Yes        -          -       Ok
    4   PSU Power Input                         Yes        -          -       Ok

    Resource ID: 11  Name: Fan Tray A (AT-FAN08)
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                          Yes        -          -       Ok

    Resource ID: 12  Name: Fan Tray B (AT-FAN08)
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                          Yes        -          -       Ok

    Resource ID: 100  Name: AT-SBx908 GEN2
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Voltage: 2.5V (Volts)                 2.487      2.344      2.865     Ok
    2   Voltage: Battery (Volts)              3.150      2.700      3.586     Ok
    3   Voltage: 3.3V (Volts)                 3.300      2.973      3.627     Ok
    4   Voltage: 12.0V (Volts)               12.125     10.813     13.188     Ok
    5   Voltage: 1.0V (Volts)                 0.998      0.900      1.097     Ok
    6   Temp: Internal (Degrees C)               34   70(Hyst)         75     Ok
    7   Temp: Fan Tray A 1 (Degrees C)           31         -5         70     Ok
    8   Temp: Fan Tray A 2 (Degrees C)           29         -5         70     Ok
    9   Temp: Fan Tray B 1 (Degrees C)           30         -5         70     Ok
    10  Temp: Fan Tray B 2 (Degrees C)           31         -5         70     Ok
    11  Temp: Near Switch (Degrees C)            34   70(Hyst)         75     Ok
    12  Temp: Front Left (Degrees C)             30   65(Hyst)         70     Ok
    13  Temp: Front Mid (Degrees C)              29   65(Hyst)         70     Ok
    14  Temp: Front Right (Degrees C)            30   65(Hyst)         70     Ok
    15  Temp: Console (Degrees C)                32   55(Hyst)         60     Ok

    Resource ID: 101  Name: AT-XEM2-12XT  Bay: 1
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Temp: XEM Front (Degrees C)              29   55(Hyst)         60     Ok
    2   Temp: XEM Rear (Degrees C)               37   70(Hyst)         75     Ok

    Resource ID: 111  Name: AT-FAN08
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Fan:  Fan Tray A 1 Int (Rpm)           4072       3000        -       Ok
    2   Fan:  Fan Tray A 1 Ext (Rpm)           3651       3000        -       Ok
    3   Fan:  Fan Tray A 2 Int (Rpm)           3997       3000        -       Ok
    4   Fan:  Fan Tray A 2 Ext (Rpm)           3624       3000        -       Ok

    Resource ID: 112  Name: AT-FAN08
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Fan:  Fan Tray B 1 Int (Rpm)           4215       3000        -       Ok
    2   Fan:  Fan Tray B 1 Ext (Rpm)           3846       3000        -       Ok
    3   Fan:  Fan Tray B 2 Int (Rpm)           4238       3000        -       Ok
    4   Fan:  Fan Tray B 2 Ext (Rpm)           3629       3000        -       Ok

    ...

Note

上記表示は一例です。表示される内容は製品、バージョン、機器構成などによって異なります。

## 注意・補足事項

VCSマスターに対して本コマンドを実行した場合は、すべてのスタックメンバーに関する情報を表示する。

## 関連コマンド