# show dot1x supplicant

モード
  特権EXECモード
カテゴリー
  インターフェース / ポート認証

## 構文

コマンド構文

`# show dot1x supplicant [interface IFRANGE] [brief]`

`# show dot1x [interface IFRANGE] supplicant [brief]`

## コマンド説明

各スイッチポートにおけるIEEE 802.1X認証（ポート認証）のSupplicant情報を表示する。

## パラメーター

`interface IFRANGE`
  スイッチポートのインターフェース名。指定したスイッチポートの情報だけを表示させたいときに指定する。ハイフン、カンマを使った複数指定も可能。省略時はすべてのインターフェースが対象となる
`brief`
  Supplicantの情報を簡素な形式で表示する

## 使用例

    awplus# show dot1x supplicant
    Interface port1.0.1
      authenticationMethod: dot1x
      totalSupplicantNum: 1
      authorizedSupplicantNum: 1
        macBasedAuthenticationSupplicantNum: 0
        dot1xAuthenticationSupplicantNum: 1
        webBasedAuthenticationSupplicantNum: 0
        otherAuthenticationSupplicantNum: 0

      Supplicant name: aaaa
      Supplicant address: 0013.3b0c.6c2b
        authenticationMethod: 802.1X
        portStatus: Authorized - currentId: 10
        abort:F fail:F start:F timeout:F success:T
        PAE: state: Authenticated - portMode: Auto
        PAE: reAuthCount: 0 - rxRespId: 0
        PAE: quietPeriod: 60 - maxReauthReq: 2
        BE: state: Idle - reqCount: 0 - idFromServer: 9
        CD: adminControlledDirections: in - operControlledDirections: in
        CD: bridgeDetected: false
        KR: rxKey: false
        KT: keyAvailable: false - keyTxEnabled: false
        RADIUS server group (auth): radius
        RADIUS server (auth): 192.168.1.5
        DHCP: IP:192.168.1.2 netmask:255.255.255.0 gateway:192.168.1.1 lease:360

    awplus# show dot1x supplicant brief
    Interface port1.0.1
      authenticationMethod: dot1x
      totalSupplicantNum: 1
      authorizedSupplicantNum: 1
        macBasedAuthenticationSupplicantNum: 0
        dot1xAuthenticationSupplicantNum: 1
        webBasedAuthenticationSupplicantNum: 0
        otherAuthenticationSupplicantNum: 0

    Interface   VID  Mode MAC Address    Status            IP Address      Username
    =========== ==== ==== ============== ================= =============== ========
    port1.0.1   1    D    0013.3b0c.6c2b Authenticated     --              aaaa

    awplus# show dot1x supplicant interface port1.0.1
    Interface port1.0.1
      authenticationMethod: dot1x
      totalSupplicantNum: 1
      authorizedSupplicantNum: 1
        macBasedAuthenticationSupplicantNum: 0
        dot1xAuthenticationSupplicantNum: 1
        webBasedAuthenticationSupplicantNum: 0
        otherAuthenticationSupplicantNum: 0

      Supplicant name: aaaa
      Supplicant address: 0013.3b0c.6c2b
        authenticationMethod: 802.1X
        portStatus: Authorized - currentId: 10
        abort:F fail:F start:F timeout:F success:T
        PAE: state: Authenticated - portMode: Auto
        PAE: reAuthCount: 0 - rxRespId: 0
        PAE: quietPeriod: 60 - maxReauthReq: 2
        BE: state: Idle - reqCount: 0 - idFromServer: 9
        CD: adminControlledDirections: in - operControlledDirections: in
        CD: bridgeDetected: false
        KR: rxKey: false
        KT: keyAvailable: false - keyTxEnabled: false
        RADIUS server group (auth): radius
        RADIUS server (auth): 192.168.1.40

    awplus# show dot1x supplicant interface port1.0.1 brief
    Interface port1.0.1
      authenticationMethod: dot1x
      totalSupplicantNum: 1
      authorizedSupplicantNum: 1
        macBasedAuthenticationSupplicantNum: 0
        dot1xAuthenticationSupplicantNum: 1
        webBasedAuthenticationSupplicantNum: 0
        otherAuthenticationSupplicantNum: 0

    Interface   VID  Mode MAC Address    Status            IP Address      Username
    =========== ==== ==== ============== ================= =============== ========
    port1.0.1   1    D    0013.3b0c.6c2b Authenticated     --              aaaa

## 注意・補足事項

実際には他の認証方式のSupplicant情報も表示されるが、briefオプションなしで実行した場合、他の認証方式のSupplicantの情報は簡潔に表示される。

## 関連コマンド