# show bgp ipv6 neighbors

モード
  非特権EXECモード
カテゴリー
  IP / 経路制御（BGP）

## 構文

コマンド構文

`> show bgp ipv6 neighbors [X:X::X:X]`

## コマンド説明

（IPv6）BGPピアの詳細情報を表示する。

## パラメーター

`X:X::X:X`
  指定したBGPピアの情報だけを表示する。省略時はすべてのBGPピアが対象となる

## 使用例

    awplus> show bgp ipv6 neighbors
    BGP neighbor is 2001:db8:2222:10::5, remote AS 65050, local AS 65010, external l
    ink
      BGP version 4, remote router ID 10.10.10.5
      BGP state = Established, up for 00:01:51
      Last read 00:01:51, hold time is 90, keepalive interval is 30 seconds
      Neighbor capabilities:
        Route refresh: advertised and received (old and new)
        4-Octet ASN Capability: advertised and received
        Address family IPv6 Unicast: advertised and received
      Received 7 messages, 0 notifications, 0 in queue
      Sent 6 messages, 0 notifications, 0 in queue
      Route refresh request: received 0, sent 0
      Minimum time between advertisement runs is 30 seconds
     For address family: IPv6 Unicast
      BGP table version 4, neighbor version 4
      Index 1, Offset 0, Mask 0x2
      Community attribute sent to this neighbor (both)
      4 accepted prefixes
      3 announced prefixes

     Connections established 1; dropped 0
    Local host: 2001:db8:2222:10::1, Local port: 46991
    Foreign host: 2001:db8:2222:10::5, Foreign port: 179
    Nexthop: 10.10.10.1
    Nexthop global: 2001:db8:2222:10::1
    Nexthop local: fe80::200:cdff:fe28:747
    BGP connection: shared network

## 関連コマンド