# show system environment

モード
  非特権EXECモード
カテゴリー
  運用・管理 / システム

## 構文

コマンド構文

`> show system environment`

## コマンド説明

製品の動作環境に関する情報（環境センサーの情報）を表示する。
表示される内容は製品、バージョン、機器構成などによって異なる。

## 使用例

    awplus> show system environment
    Environment Monitoring Status

    Overall Status: Normal
    System Airflow: Front to back

    Resource ID: 2  Name: PSU Bay A (AT-PWR600)
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                          Yes        -          -       Ok
    2   Fault                                    No        -          -       Ok
    3   PSU Power Output                        Yes        -          -       Ok
    4   PSU Power Input                         Yes        -          -       Ok

    Resource ID: 3  Name: PSU Bay B ()
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                           No        -          -       Ok
    2   Fault                                    No        -          -       Ok
    3   PSU Power Output                         No        -          -       Ok
    4   PSU Power Input                          No        -          -       Ok

    Resource ID: 4  Name: Fan Bay A (AT-FAN05)
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                          Yes        -          -       Ok

    Resource ID: 5  Name: Fan Bay B (AT-FAN05)
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                          Yes        -          -       Ok

    Resource ID: 100  Name: AT-x950-28XSQ
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Voltage: 2.5V (Volts)                 2.487      2.344      2.865     Ok
    2   Voltage: Battery (Volts)              3.136      2.700      3.586     Ok
    3   Voltage: 3.3V (Volts)                 3.317      2.973      3.627     Ok
    4   Voltage: 12.0V (Volts)               12.000     10.813     13.188     Ok
    5   Voltage: 1.0V CPU (Volts)             0.998      0.900      1.097     Ok
    6   Temp: Internal (Degrees C)               36   70(Hyst)         75     Ok
    7   Temp: Fan Tray A (Degrees C)             40         -5         70     Ok
    8   Voltage: 1V Switch (Volts)            1.034      0.950      1.050     Ok
    9   Temp: Fan Tray B (Degrees C)             39         -5         70     Ok
    10  Temp: Switch Front (Degrees C)           37   65(Hyst)         70     Ok
    11  Temp: Switch Rear (Degrees C)            45   75(Hyst)         80     Ok
    12  Temp: PSU Bays (Degrees C)               37   70(Hyst)         75     Ok
    13  Temp: Console (Degrees C)                33   70(Hyst)         75     Ok

    Resource ID: 101  Name: AT-XEM2-4QS  Bay: 1
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Temp: XEM Front (Degrees C)              29   55(Hyst)         60     Ok
    2   Temp: XEM Rear (Degrees C)               33   60(Hyst)         65     Ok

    Resource ID: 102  Name: AT-PWR600
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Voltage: PSU A Vin (Volts)          100.500     90.000    264.000     Ok
    2   Voltage: PSU A Vout (Volts)          12.023     11.000     13.000     Ok
    3   Current: PSU A Iin (Amps)             0.968        -        8.703     Ok
    4   Current: PSU A Iout (Amps)            6.562        -       60.000     Ok
    5   Power: PSU A Pin (Watts)             88.000        -      750.000     Ok
    6   Power: PSU A Pout (Watts)            78.000        -      620.000     Ok
    7   Fan: PSU A (Rpm)                      13856       4000        -       Ok
    8   Temp: PSU A Intake (Degrees C)           38         -5        100     Ok
    9   Temp: PSU A Exhaust (Degrees C)          45         -5        100     Ok

    Resource ID: 104  Name: AT-FAN05
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Fan:  Fan Tray A Left (Rpm)            7142       4000        -       Ok
    2   Fan:  Fan Tray A Middle (Rpm)          7114       4000        -       Ok
    3   Fan:  Fan Tray A Right (Rpm)           6601       4000        -       Ok

    Resource ID: 105  Name: AT-FAN05
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Fan:  Fan Tray B Left (Rpm)            7346       4000        -       Ok
    2   Fan:  Fan Tray B Middle (Rpm)          7258       4000        -       Ok
    3   Fan:  Fan Tray B Right (Rpm)           7086       4000        -       Ok

Note

上記表示は一例です。表示される内容は製品、バージョン、機器構成などによって異なります。

## 注意・補足事項

VCSマスターに対して本コマンドを実行した場合は、すべてのスタックメンバーに関する情報を表示する。

## 関連コマンド