# show scada modbus tcp server connections

モード
  特権EXECモード
カテゴリー
  運用・管理 / MODBUS

## 構文

コマンド構文

`# show scada modbus tcp server connections`

## コマンド説明

MODBUS TCPサーバーに接続しているクライアントの情報を表示する。

## 使用例

MODBUS TCPサーバーに接続中のクライアント情報を表示する。

    awplus# show scada modbus tcp server connections
    Connected client 1
      IP address      : 192.168.2.200
      Port            : 37509
      Uptime          : 22
    Statistics:
      Read Requests:
        coils                :          0
        discrete inputs      :          0
        holding registers    :          2
        input registers      :          0

      Write Requests:
        single coil          :          0
        single register      :          0
        multiple coils       :          0
        multiple registers   :          0

      Other Requests         :          0

      Exceptions:
        illegal function     :          0
        illegal data address :          0
        illegal data value   :          0
        slave device failure :          0

    Connected client 2
      IP address      : 192.168.2.200
      Port            : 49201
      Uptime          : 14
    Statistics:
      Read Requests:
        coils                :          0
        discrete inputs      :          0
        holding registers    :          1
        input registers      :          0

      Write Requests:
        single coil          :          0
        single register      :          0
        multiple coils       :          0
        multiple registers   :          0

      Other Requests         :          0

      Exceptions:
        illegal function     :          0
        illegal data address :          0
        illegal data value   :          1
        slave device failure :          0

## 関連コマンド