# show vrrp counters

モード
  非特権EXECモード
カテゴリー
  IP / VRRP

## 構文

コマンド構文

`> show vrrp counters`

## コマンド説明

VRRPの統計情報を表示する

## 使用例

    awplus# show vrrp counters
    VRRP Global Counters:
     Checksum Errors .... 230
     Version Errors ..... 0
     VRID Errors ........ 230

    VRRP IPv4 counters for VR 10/vlan10:
    Master Transitions ........ 0
     Received Advertisements ... 0
     Internal Errors ........... 0
     TTL Errors ................ 0
     Received Priority 0 Pkt ... 0
     Sent Priority 0 Pkt ....... 0
     Received Invalid Type ..... 0
     Address List Errors ....... 0
     Packet Length Errors ...... 0
     Monitored Circuit Up ...... 0
     Monitored Circuit Down..... 0

    VRRP IPv4 counters for VR 100/vlan100:
    Master Transitions ........ 1
     Received Advertisements ... 1614
     Internal Errors ........... 0
     TTL Errors ................ 0
     Received Priority 0 Pkt ... 0
     Sent Priority 0 Pkt ....... 0
     Received Invalid Type ..... 0
     Address List Errors ....... 0
     Packet Length Errors ...... 0
     Monitored Circuit Up ...... 0
     Monitored Circuit Down..... 2

表 1
Checksum Errors | 無効のチェックサム値を持つVRRPパケット数
Version Errors | 正しくないバージョンのVRRPパケット数
VRID Errors | 無効なVRIDを持つVRRPパケット数
Master Transitions | 仮想ルーターがマスターになった回数
Received Advertisements | 受信したVRRP Advertisementsの数
Internal Errors | 送信間隔のことなるVRRP Advertisementsの数
TTL Errors | TTLを持つ仮想ルーターが受信したVRRPパケットの数
Received Priority 0 Pkt | 受信したプライオリティー0のVRRPパケットの数
Sent Priority 0 Pkt | 送信したプライオリティー0のVRRPパケットの数
Received Invalid Type | 無効な値を備えたVRRPパケットの受信数
Address List Errors | アドレスリストと一致しないVRRPパケットの受信数
Packet Length Errors | ヘッダーの長さが足りないパケットの受信数
Monitored Circuit Up | Upイベントの生成数
Monitored Circuit Down | Downイベントの生成数

## 注意・補足事項

本機能の設定を行う際は、あらかじめVRRPサービスを有効にしておくこと（service vrrpコマンド）。

## 関連コマンド