# show dot1x

モード
  特権EXECモード
カテゴリー
  インターフェース / ポート認証

## 構文

コマンド構文

`# show dot1x [interface [IFRANGE]|all]`

## コマンド説明

IEEE 802.1X認証（ポート認証）の全般的情報、および、スイッチポートごとの情報を表示する。
オプションを指定せずに実行した場合は、802.1X認証の全般的情報だけが表示される。
interfaceパラメーターを指定した場合は、インターフェースごとの情報だけが表示される。
allオプションを指定した場合は、全般的設定とすべてのインターフェースごとの情報が表示される。

## パラメーター

`interface [IFRANGE]`
  スイッチポートごとの情報を表示する。特定ポートの情報だけを表示させたいときは、IFRANGEにスイッチポートのインターフェース名を指定する。ハイフン、カンマを使った複数指定も可能。省略時はポート認証の設定が行われているすべてのインターフェースが対象になる
`all`
  システム全体の情報に加え、スイッチポートごとの情報も表示させたいときに指定する

## 使用例

    awplus# show dot1x
    802.1X Port-Based Authentication Enabled
    MAC-based Port Authentication Enabled
    WEB-based Port Authentication Enabled
      RADIUS server address (auth): 172.16.10.186:1812
        Last radius message id: 22
      RADIUS server address (acct): 172.16.10.186:1813
        Last radius message id: 7

    awplus# show dot1x all
    802.1X Port-Based Authentication Enabled
    MAC-based Port Authentication Enabled
    WEB-based Port Authentication Enabled
      RADIUS server address (auth): 172.16.10.186:1812
        Last radius message id: 22
      RADIUS server address (acct): 172.16.10.186:1813
        Last radius message id: 7
    Authentication Info for interface port1.0.1
      portEnabled: true - portControl: Auto
      portStatus: Authorized
      reAuthenticate: disabled
      reAuthPeriod: 3600
      PAE: quietPeriod: 60 - maxReauthReq: 2 - txPeriod: 30
      PAE: connectTimeout: 30
      BE: suppTimeout: 30 - serverTimeout: 30 - maxReq: 2
      CD: adminControlledDirections: in
      KT: keyTxEnabled: false
      critical: disabled
      guestVlan: disabled
      authFailVlan: disabled
      dynamicVlanCreation: disabled
      hostMode: single-host
      dot1x: enabled
        protocolVersion: 1
      authMac: disabled
      authWeb: disabled
      twoStepAuthentication:
        configured: disabled
        actual: disabled
      supplicantMac: none
      Supplicant name: aaaa
      Supplicant address: 0013.3b0c.6c2b
        authenticationMethod: 802.1X
        portStatus: Authorized - currentId: 10
        abort:F fail:F start:F timeout:F success:T
        PAE: state: Authenticated - portMode: Auto
        PAE: reAuthCount: 0 - rxRespId: 0
        PAE: quietPeriod: 60 - maxReauthReq: 2
        BE: state: Idle - reqCount: 0 - idFromServer: 9
        CD: adminControlledDirections: in - operControlledDirections: in
        CD: bridgeDetected: false
        KR: rxKey: false
        KT: keyAvailable: false - keyTxEnabled: false
        RADIUS server group (auth): radius
        RADIUS server (auth): 192.168.1.5

    awplus# show dot1x interface port1.0.1
    Authentication Info for interface port1.0.1
      portEnabled: true - portControl: Auto
      portStatus: Authorized
      reAuthenticate: disabled
      reAuthPeriod: 3600
      PAE: quietPeriod: 60 - maxReauthReq: 2 - txPeriod: 30
      PAE: connectTimeout: 30
      BE: suppTimeout: 30 - serverTimeout: 30 - maxReq: 2
      CD: adminControlledDirections: in
      KT: keyTxEnabled: false
      critical: disabled
      guestVlan: disabled
      authFailVlan: disabled
      dynamicVlanCreation: disabled
      hostMode: single-host
      dot1x: enabled
        protocolVersion: 1
      authMac: disabled
      authWeb: disabled
      twoStepAuthentication:
        configured: disabled
        actual: disabled
      supplicantMac: none

## 関連コマンド