# show ethernet cfm maintenance-points local mep

モード
  特権EXECモード
カテゴリー
  L2スイッチング / イーサネットCFM（IEEE 802.1ag）

## 構文

コマンド構文

`# show ethernet cfm maintenance-points local mep {interface IFNAME [counters] | domain NAME service NAME {counters | mep <1-8191> {details | counters}}}`

## コマンド説明

ローカルMEP（メンテナンスエンドポイント）の設定とステータスを表示する。

## パラメーター

`interface IFNAME`
  インターフェース名
`counters`
  統計情報を表示する
`domain NAME`
  MDインスタンス名
`service NAME`
  MAインスタンス名
`mep <1-8191>`
  ローカルMEPインスタンスのMEP ID
`details`
  詳細を表示する

## 使用例

    awplus# show ethernet cfm maintenance-points local mep interface port1.0.2

    Service Name                      MEPID  Dir  Interface  State  Defect
    ----------------------------------------------------------------------
    MA-INST1-1                        12     D    port1.0.2  En     ..3..

    awplus# show ethernet cfm maintenance-points local mep interface port1.0.2 counters

    CFM Service Name                  MEPID    OOS-CCMs   Sent-CCMs
    ---------------------------------------------------------------
    MA-INST1-1                           12           0     1203075

    awplus# show ethernet cfm maintenance-points local mep domain MD-INST1 service MA-INST1-1 mep 12 counters

    Maintenance Points Local MEP Counters
    Domain Name..................... MD-INST1
    MA Service Name................. MA-INST1-1
    MA Service VLAN................. 0
    MEP ID.......................... 12
    Direction....................... DOWN
    Interface....................... port1.0.2
       Tx CCM Count................. 1205761
       Rx Out-of-Sequence CCM....... 0

    awplus# show ethernet cfm maintenance-points local mep domain MD-INST1 service MA-INST1-1 mep 12 details

     Domain Name....................... MD-INST1
     MA Service Name................... MA-INST1-1
     MA Primary VLAN................... 100
     MEP ID............................ 12
     Direction......................... Down
     Interface......................... port1.0.2
         MEP Active State.............. True
         CC State...................... Enabled
         CC Type....................... Multicast
         PDU VLAN Priority............. 7
         MAC-address................... 000c.2526.95a1
         Tx-RDI........................ True
         Current Defects............... 3 (someRMEPCCMdefect)
         Current Highest Defect Alarm.. 3 (someRMEPCCMdefect)
         Alarm Minimum Defect.......... 2 (someMACstatusDefect)
         Alarm Trip Time............... AUTO (2.5 seconds)
         Alarm Reset Time.............. AUTO (10 seconds)
         Configured Remote MEPs........ 21
         Missing Remote MEPs........... 21
         Error CCM Reason.............. N/A
         Last Error CCM................ N/A
         Cross-connect Defect Reason... N/A
         Last Cross Connect CCM........ N/A

## 注意・補足事項

本機能の設定を行う際は、あらかじめONMサービスを有効にしておくこと（service onmコマンド）。

## 関連コマンド