# show ipv6 mld interface

モード
  非特権EXECモード
カテゴリー
  IPv6マルチキャスト / MLD Snooping

## 構文

コマンド構文

`> show ipv6 mld interface [IFNAME]`

## コマンド説明

インターフェースのMLD関連情報を表示する。

## パラメーター

`IFNAME`
  インターフェース名。省略時はすべてのインターフェースが対象となる

## 使用例

    awplus> show ipv6 mld interface

    Interface vlan1 (Index 301)
      Child interfaces:
        port1.0.1 (A) port1.0.2 (A) port1.0.3 (N) port1.0.4 (N) ...
      Downstream interfaces:
        port1.0.2 port1.0.1
     MLD Disabled, Active(Snoop Only), Non-Querier, Version 2 (default)
     Internet address is fe80::200:f4ff:fe27:75c2
     MLD interface has 2 group-record states
     MLD activity: 3 joins, 1 leaves
     MLD querying router is fe80::200:ebff:fe0b:55b1
     MLD robustness variable is 2
     MLD last member query count is 2
     MLD query interval is 125 seconds
     MLD querier timeout is 255 seconds
     MLD max query response time is 10 seconds
     Last member query response interval is 1000 milliseconds
     Group Membership interval is 260 seconds
     MLD Snooping is globally enabled
     MLD Snooping is enabled on this interface
     MLD Snooping fast-leave is not enabled
     MLD Snooping querier is not enabled
     MLD Snooping report suppression is enabled

## 関連コマンド