# show ip prefix-list

モード
  非特権EXECモード
カテゴリー
  IP / 経路制御（フィルタリング）

## 構文

コマンド構文

`> show ip prefix-list PLISTNAME`

`> show ip prefix-list [detail|summary] [PLISTNAME]`

## コマンド説明

IPプレフィックスリストを表示する。

## パラメーター

`PLISTNAME`
  IPプレフィックスリスト名
`detail`
  詳細情報を表示させたいときに指定する
`summary`
  サマリー情報を表示させたいときに指定する

## 使用例

オプション無指定時

    awplus> show ip prefix-list
    ip prefix-list pDeny1620: 2 entries
         seq 5 deny 172.16.20.0/24
         seq 10 permit any
    ip prefix-list pDenyTen: 2 entries
       Description: Discard 10.0.0.0/8 prefixes.
         seq 5 deny 10.0.0.0/8 le 32
         seq 10 permit any

summaryオプション指定時

    awplus> show ip prefix-list summary
    Prefix-list with the last deletion/insertion: pDeny1620
    ip prefix-list pDeny1620:
       count: 2, range entries: 0, sequences: 5 - 10
    ip prefix-list pDenyTen:
       Description: Discard 10.0.0.0/8 prefixes.
       count: 2, range entries: 0, sequences: 5 - 10

detailオプション指定時

    awplus> show ip prefix-list detail
    Prefix-list with the last deletion/insertion: pDeny1620
    ip prefix-list pDeny1620:
       count: 2, range entries: 0, sequences: 5 - 10
        ripd:
         seq 5 deny 172.16.20.0/24 (hit count: 10, refcount: 20)
         seq 10 permit any (hit count: 10, refcount: 10)
        ospfd:
         seq 5 deny 172.16.20.0/24 (hit count: 0, refcount: 0)
         seq 10 permit any (hit count: 0, refcount: 0)
    ip prefix-list pDenyTen:
       Description: Discard 10.0.0.0/8 prefixes.
       count: 2, range entries: 0, sequences: 5 - 10
        ripd:
         seq 5 deny 10.0.0.0/8 le 32 (hit count: 28, refcount: 140)
         seq 10 permit any (hit count: 168, refcount: 168)
        ospfd:
         seq 5 deny 10.0.0.0/8 le 32 (hit count: 0, refcount: 0)
         seq 10 permit any (hit count: 0, refcount: 0)

## 関連コマンド