# show ipv6 mroute

モード
  非特権EXECモード
カテゴリー
  IPv6マルチキャスト / 一般設定

## 構文

コマンド構文

`> show ipv6 mroute [ADDRESSES] [count|summary]`

## コマンド説明

IPv6マルチキャスト経路表（マルチキャスト配送ツリーの情報）を表示する。

## パラメーター

`ADDRESSES`
  IPv6アドレス。次のいずれかの形式で指定する。指定時は指定したアドレスと合致するエントリーだけを表示する。省略時はすべてのエントリーを表示する
  `GROUP := X:X::X:X`
    マルチキャストグループアドレス
  `SOURCE := X:X::X:X`
    マルチキャスト送信者のIPv6アドレス
  `GROUP SOURCE := X:X::X:X X:X::X:X`
    マルチキャストグループアドレスとマルチキャスト送信者のIPv6アドレス
  `SOURCE GROUP := X:X::X:X X:X::X:X`
    マルチキャスト送信者のIPv6アドレスとマルチキャストグループアドレス
`count|summary`
  統計情報を表示（count）するかサマリー情報を表示（summary）するかを選択する。省略時は各エントリーの内容を表示する

## 使用例

    awplus# show ipv6 mroute
    IPv6 Multicast Routing Table
    Flags: I - Immediate Stat, T - Timed Stat, F - Forwarder
    installed
    Timers: Uptime/Stat Expiry
    Interface State: Interface
    (2001:db8:10:10::feed, ff1e::beaf), uptime 03:18:38
    Owner IMI, Flags: F
      Incoming interface: vlan10
      Outgoing interface list:
        vlan20

    awplus# show ipv6 mroute count

    IPv6 Multicast Statistics
    Total 1 routes using 152 bytes memory
    Route limit/Route threshold: 1024/1024
    Total NOCACHE/WRONGmif/WHOLEPKT recv from fwd: 6/0/0
    Total NOCACHE/WRONGmif/WHOLEPKT sent to clients: 6/0/0
    Immediate/Timed stat updates sent to clients: 0/0
    Reg ACK recv/Reg NACK recv/Reg pkt sent: 0/0/0
    Next stats poll: 00:01:14

    Forwarding Counts: Pkt count/Byte count, Other Counts: Wrong If
    pkts
    Fwd msg counts: WRONGmif/WHOLEPKT recv
    Client msg counts: WRONGmif/WHOLEPKT/Imm Stat/Timed Stat sent
    Reg pkt counts: Reg ACK recv/Reg NACK recv/Reg pkt sent

    (2001:db8:10:10::feed, ff1e::beaf), Forwarding: 0/0, Other: 0
      Fwd msg: 0/0, Client msg: 0/0/0/0, Reg: 0/0/0

    awplus# show ipv6 mroute summary
    IPv6 Multicast Routing Table
    Flags: I - Immediate Stat, T - Timed Stat, F - Forwarder
    installed
    Timers: Uptime/Stat Expiry
    Interface State: Interface

    (2001:db8:10:10::feed, ff1e::beaf), 03:20:28/-, IMI, Flags: F

## 関連コマンド