# show wireless network

モード
  非特権EXECモード
カテゴリー
  無線LANコントローラー（AWC対応） / 無線ネットワーク設定

## 構文

コマンド構文

`> show wireless network [<1-65535>|all] [brief]`

## コマンド説明

無線ネットワークの設定内容を表示する。

## パラメーター

`<1-65535>`
  無線ネットワーク設定番号。カンマ、ハイフン区切りで複数指定が可能。本パラメーター指定時は指定したネットワークだけを表示する。省略時はallを指定したのと同じ動作となる
`all`
  すべてのネットワークを表示する（省略時動作）
`brief`
  無線ネットワークの情報を簡潔に表示させたいときに指定する。省略時は詳細な情報が表示される

## 使用例

    awplus> show wireless network
    Network ID 10:
     Description ...................
     Assigned VLAN ID .............. 10
     SSID .......................... wnet10
     Hide SSID ..................... -
     Emergency Mode ................ Disable
     Band-Steering ................. Disable
     Association Advertisement ..... Disable
     DTIM Period ................... 1
     Proxy ARP ..................... Disable
      ARP Pass Through ............. Disable
     BSS Transition Management ..... Disable
     Security ID ................... 10
      Security Mode ................ wpa-personal
     MAC-Auth
      Authentication Mode .......... radius
      RADIUS group .................
      Username
       Separator ................... hyphen
       Character Case .............. lower-case
      Password .....................
      RADIUS Send Service Type ..... Disable
      RADIUS DAC IP Address ........
      RADIUS Calling-Station-Id
       Separator ................... hyphen
       Character Case .............. upper-case
      Verify RADIUS Packets ........ Disable
      Dynamic VLAN ................. Disable
      Critical mode ................ Disable
     RADIUS group for Web-Auth .....
     Two-step authentication ....... Enable
     Wireless MAC filter ID ........ Profile
     Wireless Trigger ID ........... 0
     Inactivity Timer .............. 300
     Client Isolation Mode ......... Disabled
     Airtime Percentage ............ 0
     Multicast Unicast conversion .. Disable
     Disconnect Low-Signal Clients . Disabled
     RSSI Threshold ................ -75
     Captive portal ................ Enable
      Authentication Mode .......... click-through
      RADIUS group .................
      RADIUS Accounting ............ Disable
      External Page URL ............
      Redirect URL .................
      Session keep ................. Enable
      Session Timeout Interval ..... 3600
      Session Timeout Action . ..... Reauthentication
      Page proxy URL ...............
      Walled Garden Entries ........ 0
      DNS Proxy for Walled Garden .. Disable
      Verify RADIUS Packets ........ Disable
     Passpoint ..................... Disable

    Network ID 20:
    ...
     Passpoint ..................... Enable
      802.11u
       Access Network Type ......... public
       Internet Access ............. Enable
       Additional Step Required .... Enable
       ES Reacheable ............... Enable
       Unauth ES Accessible ........ Enable
       Venue Group ................. 7
       Venue Type .................. 1
       Homogeneous ESSID ........... 1234.5678.9abc
       Roaming Consortium List ..... 021122,02233445566
       Venue Name Information
        ID  1:
         Language Code ............. jpn
         Venue Name ................ Example venue1
        ID  2:
         Language Code ............. eng
         Venue Name ................ Example venue2
       Network Auth Type
        Auth Type .................. redirect-http-https
        Redirect URL ............... http://www.example.com/redirect/me/here
       IP Type Availability v4/v6 .. public/no-exist
       Domain Name ................. example.com,google.com
       3GPP Info (MCC,MNC) ......... 244,91;310,261
       NAI Realm Information
        ID  1:
         Realm Name ................ example.com,example.net
         EAP Method ................ EAP-TLS
        ID  2:
         Realm Name ................ example.com;example.net
         EAP Method ................ EAP-TLS,EAP-TTLS/MSCHAPv2
       ANQP-element Configuration
        Info ID    1: Payload ...... 0000
        Info ID   20: Payload ...... 00000000
       GAS Address 3 Behavior ...... 0
       GAS Comeback Delay .......... 1000
       QoS Map Set configuration ... 53,2,22,6,8,15,0,7,255,255,16,31,32,39,255,255,40,47,255,255
      Hotspot2.0
       DGAF ........................ Disable
       L2 Traf Inspect and Filter .. Disable
       ANQP Domain ID .............. 0
       Deauth Request Timeout ...... 60
       Operator Friendly Name
        ID  1:
         Language Code ............. jpn
         Friendly Name ............. TestJP
        ID  2:
         Language Code ............. eng
         Friendly Name ............. TestNZ
       Connection Capability
         IP Protocol 1:
          Port ..................... 0
          Status ................... open
         IP Protocol 12:
          Port ..................... 80
          Status ................... open
       WAN Metrics
         WAN Information ........... 01
         Speed Uplink/Downlink ..... 384/2500
         Load Uplink/Downlink ...... 0/0
         Load Measure Duration ..... 10
       Operating Class Indication .. 51

    awplus> show wireless network brief
    ID    VLAN SSID                             H E  Sec ID MAC-Auth Web-Auth
    ----- ---- -------------------------------- - -- ------ -------- --------
       10   10 wnet10                           - -      10        -        -
       20   20 wnet20                           - -      20        -        -

## 関連コマンド