# show bfd peer

モード
  特権EXECモード
カテゴリー
  IP / BFD

## 構文

コマンド構文

`# show bfd [vrf VRFNAME] peer`

`# show bfd [vrf VRFNAME] peer brief`

`# show bfd [vrf VRFNAME] peer {A.B.C.D|X:X::X:X} [multihop] [local-address {A.B.C.D|X:X::X:X}] [interface IFNAME]`

## コマンド説明

BFDピアの設定と状態を表示する。

## パラメーター

`vrf VRFNAME`
  VRFインスタンス名
`brief`
  情報を簡潔に表示する
`A.B.C.D`
  BFDピアのIPv4アドレス
`X:X::X:X`
  BFDピアのIPv6アドレス
`multihop`
  マルチホップピア
`local-address {A.B.C.D|X:X::X:X}`
  ローカルアドレス
`interface IFNAME`
  インターフェース名

## 使用例

    awplus# show bfd peer

    BFD Peers:
           peer 172.16.11.3 vrf default interface vlan101
                   ID: 2702513920
                   Remote ID: 1
                   Active mode
                   Status: up
                   Uptime: 3 hour(s), 30 minute(s), 57 second(s)
                   Diagnostics: ok
                   Remote diagnostics: ok
                   Peer Type: dynamic
                   Local timers:
                           Detect-multiplier: 3
                           Receive interval: 300ms
                           Transmission interval: 300ms
                           Echo transmission interval: 50ms
                   Remote timers:
                           Detect-multiplier: 3
                           Receive interval: 1000ms
                           Transmission interval: 1000ms
                           Echo transmission interval: 50ms

            peer 172.16.11.89 vrf default
                    ID: 377093019
                    Remote ID: 0
                    Status: down
                    Downtime: 28 minute(s), 9 second(s)
                    Diagnostics: ok
                    Remote diagnostics: ok
                    Peer Type: configured
                    Local timers:
                            Detect-multiplier: 3
                            Receive interval: 300ms
                            Transmission interval: 300ms
                            Echo transmission interval: 50ms
                    Remote timers:
                            Detect-multiplier: 3
                            Receive interval: 1000ms
                            Transmission interval: 1000ms
                            Echo transmission interval: 0ms

    awplus# show bfd peer brief

    Session count: 2
    SessionId  LocalAddress                             PeerAddress                             Status
    =========  ============                             ===========                             ======
    2702513920 172.16.11.2                              172.16.11.3                             up
    377093019  unknown                                  172.16.11.89                            down

## 関連コマンド