# show system environment

モード
  非特権EXECモード
カテゴリー
  運用・管理 / システム

## 構文

コマンド構文

`> show system environment`

## コマンド説明

製品の動作環境に関する情報（環境センサーの情報）を表示する。
表示される内容は製品、バージョン、機器構成などによって異なる。

## 使用例

    awplus> show system environment
    Environment Monitoring Status

    Overall Status: Normal

    Resource ID: 3  Name: PSU Bay 1 (AT-PWRSYS4)
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                          Yes        -          -       Ok
    2   Fault                                    No        -          -       Ok
    3   PSU Power Output                        Yes        -          -       Ok

    Resource ID: 4  Name: PSU Bay 2 (AT-PWRSYS4)
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                          Yes        -          -       Ok
    2   Fault                                    No        -          -       Ok
    3   PSU Power Output                        Yes        -          -       Ok

    Resource ID: 5  Name: Fan Tray 1 (AT-FAN17)
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                          Yes        -          -       Ok

    Resource ID: 6  Name: Fan Tray 2 (AT-FAN17)
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                          Yes        -          -       Ok

    Resource ID: 7  Name: Fan Tray 3 (AT-FAN17)
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                          Yes        -          -       Ok

    Resource ID: 8  Name: Fan Tray 4 (AT-FAN17)
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                          Yes        -          -       Ok

    Resource ID: 9  Name: Fan Tray 5 (AT-FAN17)
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Device Present                          Yes        -          -       Ok

    Resource ID: 100  Name: AT-x980-32CQ
    ID  Sensor (Units)                      Reading  Low Limit High Limit Status
    1   Temp: CPU (Degrees C)                    49   87(Hyst)         92     Ok
    2   Temp: PSU-1 Intake (Degrees C)           32   71(Hyst)         76     Ok
    3   Temp: PSU-2 Intake (Degrees C)           25   45(Hyst)         50     Ok
    4   Temp: MAC Heatsink (Degrees C)           28   46(Hyst)         51     Ok
    5   Temp: Ambient (Degrees C)                25   42(Hyst)         47     Ok
    6   Temp: Fan Board (Degrees C)              25   48(Hyst)         53     Ok
    7   Voltage: 12V (Volts)                 11.976     10.799     13.200     Ok
    8   Voltage: 5.0V (Volts)                 4.986      4.500      5.500     Ok
    9   Voltage: 3.3V (Volts)                 3.320      2.969      3.629     Ok
    10  Voltage: 3.3V (Volts)                 3.268      2.969      3.629     Ok
    11  Voltage: 1.8V (Volts)                 1.788      1.619      1.979     Ok
    12  Voltage: 1.1V (Volts)                 1.083      0.989      1.210     Ok
    13  Voltage: 0.865V (Volts)               0.882      0.765      0.934     Ok
    14  Voltage: 0.8V (Volts)                 0.802      0.719      0.880     Ok
    15  Voltage: 0.9V (Volts)                 0.919      0.765      1.034     Ok
    16  Fan: Fan 1-1 (Rpm)                     8280       7000        -       Ok
    17  Fan: Fan 1-2 (Rpm)                     7440       7000        -       Ok
    18  Fan: Fan 2-1 (Rpm)                     8400       7000        -       Ok
    19  Fan: Fan 2-2 (Rpm)                     7440       7000        -       Ok
    20  Fan: Fan 3-1 (Rpm)                     8520       7000        -       Ok
    21  Fan: Fan 3-2 (Rpm)                     7440       7000        -       Ok
    22  Fan: Fan 4-1 (Rpm)                     8520       7000        -       Ok
    23  Fan: Fan 4-2 (Rpm)                     7440       7000        -       Ok
    24  Fan: Fan 5-1 (Rpm)                     8400       7000        -       Ok
    25  Fan: Fan 5-2 (Rpm)                     7440       7000        -       Ok

Note

上記表示は一例です。表示される内容は製品、バージョン、機器構成などによって異なります。

## 注意・補足事項

VCSマスターに対して本コマンドを実行した場合は、すべてのスタックメンバーに関する情報を表示する。

## 関連コマンド