# show ip igmp interface

モード
  非特権EXECモード
カテゴリー
  IPマルチキャスト / IGMP Snooping

## 構文

コマンド構文

`> show ip igmp [vrf VRFNAME|global] interface [IFNAME]`

## コマンド説明

インターフェースのIGMP関連情報を表示する。

## パラメーター

`vrf VRFNAME`
  VRFインスタンス名。指定したVRFインスタンスのみ表示するときに指定する
`global`
  グローバルVRFインスタンスのみ表示するときに指定
`IFNAME`
  インターフェース名。省略時はすべてのインターフェースが対象となる

## 使用例

    awplus> show ip igmp interface vlan1
    Interface vlan1 (Index 301)
     IGMP Disabled, Active(Snoop Only), Non-Querier, Version 3 (default)
     IGMP interface has 0 group-record states
     IGMP activity: 0 joins, 0 leaves
     IGMP querying router is 0.0.0.0
     IGMP robustness variable is 2
     IGMP last member query count is 2
     IGMP query interval is 125 seconds
     IGMP query holdtime is 500 milliseconds
     IGMP querier timeout is 255 seconds
     IGMP max query response time is 10 seconds
     Last member query response interval is 1000 milliseconds
     Group Membership interval is 260 seconds
     Strict IGMPv3 ToS checking is disabled on this interface
     Source Address checking is enabled
     Global Specific Query Flooding is enabled
     IGMP Snooping is globally enabled
     IGMP Snooping query solicitation is globally disabled
      Num. query-solicit packets: 34 sent, 0 recvd
     IGMP Snooping is enabled on this interface
     IGMP Snooping fast-leave is not enabled
     IGMP Snooping querier is not enabled
     IGMP Snooping report suppression is enabled
     IGMP Snooping source timer is globally disabled
     IGMP Snooping source timer is disabled

## 関連コマンド