# show interface

モード
  非特権EXECモード
カテゴリー
  インターフェース / 一般設定

## 構文

コマンド構文

`> show interface [IFRANGE] [brief]`

## コマンド説明

指定したインターフェースの情報を表示する。

## パラメーター

`IFRANGE`
  インターフェース名。ハイフン、カンマを使った複数指定も可能。種類の異なるインターフェースを混在させてもよい。省略時はすべてのインターフェースが対象となる
`brief`
  インターフェースの情報を簡潔に表示させたいときに指定する。省略時は詳細な情報が表示される

## 使用例

PPP（PPPoE）インターフェースppp0の情報を表示する。

    awplus# show interface ppp0
    Interface ppp0
      Link is UP, administrative state is UP
      Hardware is PPP
      IPv4 address 10.0.0.1/32
      index xxx metric 1 mtu 1454
      <UP,POINTOPOINT,RUNNING,NOARP,MULTICAST>
      PPP is running over interface eth1
      LCP Opened IPCP Opened
      MRU(bytes): Local config 1492, Local negotiated 1492, Peer negotiated 1454
      Magic number: Local config ON, Local negotiated ON, Peer negotiated ON
      Authentication: Local config None, Local neg None, Peer neg CHAP
      Echo Request Timer (seconds): 10
      IPv4 addresses: Local config 0.0.0.0
                      Local neg 10.0.0.1, Peer neg 10.0.0.2
      Local DNS addresses: 10.0.0.10, 10.0.0.100
      IPv6 Id Local config: 0000:0000:0000:0000
      PPPoE is using the default service
      SNMP link-status traps: Disabled
        input packets 3, bytes 54, dropped 3, multicast packets 0
        output packets 3, bytes 54, multicast packets 0 broadcast packets 0
        input average rate : 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        output average rate: 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        input peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
        output peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
      Time since last state change: 0 days 00:00:30

IPsecトンネルインターフェースtunnel1の情報を表示する。

    awplus# show interface tunnel1
    Interface tunnel1
      Link is UP, administrative state is UP
      Hardware is Tunnel
      IPv4 address 192.168.1.1/30 pointopoint 192.168.1.3
      index xxx metric 1 mtu 1480
      arp ageing timeout 300

      SNMP link-status traps: Disabled
      Tunnel source 10.1.0.10, destination 10.2.0.10
      Tunnel local 10.1.0.10, remote 10.2.0.10
      Tunnel protocol/transport ipsec ipv4, key disabled, sequencing disabled
      Tunnel TTL inherit
      Checksumming of packets disabled, path MTU discovery disabled
      Tunnel protection via IPsec (profile "default")
        input packets 11, bytes 924, dropped 0, multicast packets 0
        output packets 0, bytes 0, multicast packets 0 broadcast packets 0
        input average rate : 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        output average rate: 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        input peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
        output peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
      Time since last state change: 0 days 03:23:10

L2TPv3トンネルインターフェースtunnel0の情報を表示する。

    awplus> show interface tunnel0
    Interface tunnel0
      Link is UP, administrative state is UP
      Hardware is Tunnel
      index xxx metric 1 mtu 1488
      Bridge-group 1 (br1)
      <UP,BROADCAST,RUNNING,MULTICAST>
      SNMP link-status traps: Disabled
      Tunnel source 10.1.1.1, destination 10.1.1.2
      Tunnel name local 10.1.1.1, remote 10.1.1.2
      Tunnel ID local 101, remote 102
      Tunnel protocol/transport l2tp v3, key disabled, sequencing disabled
      Tunnel TTL -
      Checksumming of packets disabled, path MTU discovery disabled
        input packets 0, bytes 0, dropped 0, multicast packets 0
        output packets 0, bytes 0, multicast packets 0 broadcast packets 0
        input average rate : 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        output average rate: 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        input peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
        output peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
      Time since last state change: 0 days 00:01:32

802.1Q L2TPv3トンネルサブインターフェースtunnel0.10の情報を表示する。

    awplus> show interface tunnel0.10
    Interface tunnel0.10
      Link is UP, administrative state is UP
      Hardware is Encapsulated Ethernet, address is XXXX.XXXX.XXXX
      index xxx metric 1 mtu 1488
      802.1Q VID 10 over tunnel0
      Bridge-group 11 (br11)
      <UP,BROADCAST,RUNNING,MULTICAST>
      SNMP link-status traps: Disabled
        input packets 0, bytes 0, dropped 0, multicast packets 0
        output packets 0, bytes 0, multicast packets 0 broadcast packets 0
        input average rate : 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        output average rate: 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        input peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
        output peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
      Time since last state change: 0 days 02:21:54

OpenVPN Tap(L2)トンネルインターフェースtunnel0の情報を表示する。

    awplus> show interface tunnel0
    Interface tunnel0
      Link is UP, administrative state is UP
      Hardware is Tunnel
      IPv4 address 192.168.1.1/24 broadcast 192.168.1.255
      index xxx metric 1 mtu 1500
      <UP,BROADCAST,RUNNING,MULTICAST>
      SNMP link-status traps: Disabled
      Tunnel source UNKNOWN, destination UNKNOWN
      Tunnel name local awplus, remote  UNKNOWN
      Tunnel ID local (not set), remote (not set)
      Tunnel protocol/transport openvpn tap, key disabled, sequencing disabled
      Tunnel TTL -
      Tunnel RADIUS servers:
        host 127.0.0.1, port 1812
      Checksumming of packets disabled, path MTU discovery disabled
        input packets 202, bytes 23009, dropped 0, multicast packets 0
        output packets 6, bytes 360, multicast packets 0 broadcast packets 0
        input average rate : 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        output average rate: 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        input peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
        output peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
      Time since last state change: 0 days 00:01:34

OpenVPN Tun(L3)トンネルインターフェースtunnel0の情報を表示する。

    awplus# show interface tunnel0
    Interface tunnel0
      Link is UP, administrative state is UP
      Hardware is Tunnel
      IPv4 address 192.168.1.1/24 pointopoint 192.168.1.255
      index xxx metric 1 mtu 1500
      <UP,POINTOPOINT,RUNNING,MULTICAST>
      SNMP link-status traps: Disabled
      Tunnel source UNKNOWN, destination UNKNOWN
      Tunnel name local awplus, remote  UNKNOWN
      Tunnel ID local (not set), remote (not set)
      Tunnel protocol/transport openvpn tun, key disabled, sequencing disabled
      Tunnel TTL -
      Checksumming of packets disabled, path MTU discovery disabled
        input packets 0, bytes 0, dropped 0, multicast packets 0
        output packets 6, bytes 360, multicast packets 0 broadcast packets 0
        input average rate : 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        output average rate: 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        input peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
        output peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
      Time since last state change: 0 days 00:01:14

GREトンネルインターフェースtunnel10の情報を表示する。

    awplus> show interface tunnel10
    Interface tunnel10
      Link is UP, administrative state is UP
      Hardware is Tunnel
      IPv6 address 2001:db8:10:10::1/64
      IPv6 address fe80::21a:ebff:fe92:a4bc/64
      index xxx metric 1 mtu 1476
      <UP,POINTOPOINT,RUNNING,MULTICAST>
      SNMP link-status traps: Disabled
      Tunnel source 10.1.1.1, destination 10.1.1.2
      Tunnel name local 10.1.1.1, remote 10.1.1.2
      Tunnel ID local (not set), remote (not set)
      Tunnel protocol/transport gre, key disabled, sequencing disabled
      Tunnel TTL 64
      Checksumming of packets disabled, path MTU discovery disabled
        input packets 0, bytes 0, dropped 0, multicast packets 0
        output packets 8, bytes 480, multicast packets 0 broadcast packets 0
        input average rate : 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        output average rate: 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        input peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
        output peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
      Time since last state change: 0 days 00:01:29

IPv4 over IPv6トンネルインターフェースtunnel1の情報を表示する。

    awplus> show interface tunnel1
    Interface tunnel1
      Link is UP, administrative state is UP
      Hardware is Tunnel
      IPv4 address 172.16.10.1/24 pointopoint 172.16.10.255
      index xxx metric 1 mtu 1460
      <UP,POINTOPOINT,RUNNING,MULTICAST>
      SNMP link-status traps: Disabled
      Tunnel source 2001:db8:1:1::1, destination 2001:db8:1:1::2
      Tunnel name local 2001:db8:1:1::1, remote 2001:db8:1:1::2
      Tunnel ID local (not set), remote (not set)
      Tunnel protocol/transport ipv6, key disabled, sequencing disabled
      Tunnel TTL 64
      Checksumming of packets disabled, path MTU discovery disabled
        input packets 0, bytes 0, dropped 0, multicast packets 0
        output packets 0, bytes 0, multicast packets 0 broadcast packets 0
        input average rate : 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        output average rate: 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        input peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
        output peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
      Time since last state change: 0 days 00:17:23

表 1：詳細表示（briefオプション未指定時）
Interface | インターフェース名
Link is | リンクステータス
administrative state is | 管理ステータス。UP（ポートが有効に設定されている）、DOWN（ポートが無効に設定されている）、err-disabled（製品の機能によりポートがブロックされてリンクダウンしている）
Thrash-limiting | 未サポート
Hardware is | インターフェース種別。Ethernet、Loopback、Tunnelなどがある
address is | 物理（MAC）アドレス
DHCP client enabled on interface | 該当インターフェースでDHCPクライアント機能が有効な場合に表示される
IPv4 address | IPアドレス/マスク長。IPアドレスが設定されているときだけ表示される
broadcast | IPブロードキャストアドレス。IPアドレスが設定されているときだけ表示される
IPv6 address | IPv6アドレス/プレフィックス長。IPv6アドレスが設定されているときだけ表示される。該当アドレスの状態がpreferred（優先アドレス）以外の場合は、行末にtentative（暫定アドレス）、DAD failed（暫定アドレスの重複を検出）、deprecated（非推奨アドレス）のいずれかの状態が表示される。また、状態のあとにアスタリスク（*）が表示されている場合、該当アドレスが自動設定されたことを示す。IPv6アドレスの状態についてはshow ipv6 interfaceコマンドのページを参照
Description | インターフェースの説明文
index | インターフェースインデックス番号（ifIndex）
current duplex | 実際のデュプレックスモード。物理インターフェース（eth、port）にだけ表示される
current speed | 実際の通信速度。物理インターフェース（eth、port）にだけ表示される
polarity | 極性。物理インターフェース（eth、port）にだけ表示される
configured duplex | デュプレックスモードの設定値。物理インターフェース（eth、port）にだけ表示される
configured speed | 通信速度の設定値。物理インターフェース（eth、port）にだけ表示される
metric | メトリック
mtu | MTU（Maximum Transmission Unit）
mru | MRU（Maximum Receive Unit）
arp ageing timeout | ARPタイムアウト（ARPエントリー保持時間）
<UP,BROADCAST,RUNNING,MULTICAST> | インターフェースフラグの状態
SNMP link-status traps | SNMPのリンクステータス通知メッセージを生成するかどうか。Sending（生成する）、Disabled（生成しない）のいずれか。Sendingに設定されており、なおかつ、単位時間あたりの生成数に上限が設定されている場合は「(suppressed after 20 traps in 30 sec)」のような形式で上限値も表示される。上限が設定されていない場合は「(suppression disabled)」と表示される
input packets | 受信パケット数。以下、受信パケットに関して、bytes（バイト数）、dropped（破棄パケット数）、multicast packets（マルチキャストパケット数）が表示される
output packets | 送信パケット数。以下、送信パケットに関して、bytes（バイト数）、multicast packets（マルチキャストパケット数）、broadcast packets（ブロードキャストパケット数）が表示される
Time since last state change | 前回ステータス変更後の経過時間

表 2：簡潔表示（briefオプション指定時）
Interface | インターフェース名
Status | 管理ステータス
Protocol | リンクステータス

## 注意・補足事項

各インターフェースのインターフェースインデックス番号（ifIndex）は次のとおり。

表 1
インターフェース種別 | インターフェースインデックス番号（ifIndex）
ループバックインターフェース（lo） | 1
PPPインターフェース（pppX） | 利用可能な番号が内部で自動的に割り当てられる。 ただし、トンネルインターフェースについては、トンネル種別に応じた必要最低限の設定をしないとifIndexは割り当てられない
VAPインターフェース（vapX.Y）
Ethernetインターフェース（ethX）
ボンドインターフェース（bondX）
ブリッジインターフェース（brX）
トンネルインターフェース（tunnelX）
802.1Qサブインターフェース（ethX.Y、bondX.Y、tunnelX.Y、br0.Y）

Note

以下のインターフェースは、起動時にインターフェースインデックス番号を採番するため、作成時と異なる場合があります。

- VAPインターフェース（vapX.Y）
- Ethernetインターフェース（ethX）
- PPPインターフェース（pppX）
- ボンドインターフェース（bondX）
- ブリッジインターフェース（brX）
- トンネルインターフェース（tunnelX）
- 802.1Qサブインターフェース（ethX.Y、bondX.Y、tunnelX.Y、br0.Y）

トンネルインターフェース（tunnelX）と802.1Qトンネルサブインターフェース（tunnelX.Y）、PPPインターフェース（pppX）については、インターフェースダウン/アップ後にもインターフェースインデックス番号を採番するため、インターフェースダウン/アップ後にインターフェースインデックス番号が変わります。
droppedカウンターはカウントされません。
administrative stateのerr-disabledは、製品の機能によってポートがリンクダウンしている場合にのみ表示されます。このため、STPなどの機能によって、リンクアップしたままポートがブロックされている状態となった場合、err-disabledとは表示されずUPと表示されます。

## 関連コマンド