# show interface

モード
  非特権EXECモード
カテゴリー
  インターフェース / 一般設定

## 構文

コマンド構文

`> show interface [IFRANGE] [brief]`

## コマンド説明

指定したインターフェースの情報を表示する。

## パラメーター

`IFRANGE`
  インターフェース名。ハイフン、カンマを使った複数指定も可能。種類の異なるインターフェースを混在させてもよい。省略時はすべてのインターフェースが対象となる
`brief`
  インターフェースの情報を簡潔に表示させたいときに指定する。省略時は詳細な情報が表示される

## 使用例

PPP（PPPoE）インターフェースppp0の情報を表示する。

    awplus# show interface ppp0
    Interface ppp0
      Link is UP, administrative state is UP
      Hardware is PPP
      IPv4 address 10.0.0.1/32
      index xxx metric 1 mtu 1454
      <UP,POINTOPOINT,RUNNING,NOARP,MULTICAST>
      PPP is running over interface eth1
      LCP Opened IPCP Opened
      MRU(bytes): Local config 1492, Local negotiated 1492, Peer negotiated 1454
      Magic number: Local config ON, Local negotiated ON, Peer negotiated ON
      Authentication: Local config None, Local neg None, Peer neg CHAP
      Echo Request Timer (seconds): 10
      IPv4 addresses: Local config 0.0.0.0
                      Local neg 10.0.0.1, Peer neg 10.0.0.2
      Local DNS addresses: 10.0.0.10, 10.0.0.100
      IPv6 Id Local config: 0000:0000:0000:0000
      PPPoE is using the default service
      SNMP link-status traps: Disabled
        input packets 3, bytes 54, dropped 3, multicast packets 0
        output packets 3, bytes 54, multicast packets 0 broadcast packets 0
        input average rate : 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        output average rate: 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        input peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
        output peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
      Time since last state change: 0 days 00:00:30

L2TPv3トンネルインターフェースtunnel0の情報を表示する。

    awplus> show interface tunnel0
    Interface tunnel0
      Link is UP, administrative state is UP
      Hardware is Tunnel
      index xxx metric 1 mtu 1488
      Bridge-group 1 (br1)
      <UP,BROADCAST,RUNNING,MULTICAST>
      SNMP link-status traps: Disabled
      Tunnel source 10.1.1.1, destination 10.1.1.2
      Tunnel name local 10.1.1.1, remote 10.1.1.2
      Tunnel ID local 101, remote 102
      Tunnel protocol/transport l2tp v3, key disabled, sequencing disabled
      Tunnel TTL -
      Checksumming of packets disabled, path MTU discovery disabled
        input packets 0, bytes 0, dropped 0, multicast packets 0
        output packets 0, bytes 0, multicast packets 0 broadcast packets 0
        input average rate : 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        output average rate: 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        input peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
        output peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
      Time since last state change: 0 days 00:01:32

802.1Q L2TPv3トンネルサブインターフェースtunnel0.10の情報を表示する。

    awplus> show interface tunnel0.10
    Interface tunnel0.10
      Link is UP, administrative state is UP
      Hardware is Encapsulated Ethernet, address is XXXX.XXXX.XXXX
      index xxx metric 1 mtu 1488
      802.1Q VID 10 over tunnel0
      Bridge-group 11 (br11)
      <UP,BROADCAST,RUNNING,MULTICAST>
      SNMP link-status traps: Disabled
        input packets 0, bytes 0, dropped 0, multicast packets 0
        output packets 0, bytes 0, multicast packets 0 broadcast packets 0
        input average rate : 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        output average rate: 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        input peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
        output peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
      Time since last state change: 0 days 02:21:54

OpenVPN Tap(L2)トンネルインターフェースtunnel0の情報を表示する。

    awplus> show interface tunnel0
    Interface tunnel0
      Link is UP, administrative state is UP
      Hardware is Tunnel
      IPv4 address 192.168.1.1/24 broadcast 192.168.1.255
      index xxx metric 1 mtu 1500
      <UP,BROADCAST,RUNNING,MULTICAST>
      SNMP link-status traps: Disabled
      Tunnel source UNKNOWN, destination UNKNOWN
      Tunnel name local awplus, remote  UNKNOWN
      Tunnel ID local (not set), remote (not set)
      Tunnel protocol/transport openvpn tap, key disabled, sequencing disabled
      Tunnel TTL -
      Tunnel RADIUS servers:
        host 127.0.0.1, port 1812
      Checksumming of packets disabled, path MTU discovery disabled
        input packets 202, bytes 23009, dropped 0, multicast packets 0
        output packets 6, bytes 360, multicast packets 0 broadcast packets 0
        input average rate : 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        output average rate: 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        input peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
        output peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
      Time since last state change: 0 days 00:01:34

OpenVPN Tun(L3)トンネルインターフェースtunnel0の情報を表示する。

    awplus# show interface tunnel0
    Interface tunnel0
      Link is UP, administrative state is UP
      Hardware is Tunnel
      IPv4 address 192.168.1.1/24 pointopoint 192.168.1.255
      index xxx metric 1 mtu 1500
      <UP,POINTOPOINT,RUNNING,MULTICAST>
      SNMP link-status traps: Disabled
      Tunnel source UNKNOWN, destination UNKNOWN
      Tunnel name local awplus, remote  UNKNOWN
      Tunnel ID local (not set), remote (not set)
      Tunnel protocol/transport openvpn tun, key disabled, sequencing disabled
      Tunnel TTL -
      Checksumming of packets disabled, path MTU discovery disabled
        input packets 0, bytes 0, dropped 0, multicast packets 0
        output packets 6, bytes 360, multicast packets 0 broadcast packets 0
        input average rate : 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        output average rate: 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        input peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
        output peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
      Time since last state change: 0 days 00:01:14

GREトンネルインターフェースtunnel10の情報を表示する。

    awplus> show interface tunnel10
    Interface tunnel10
      Link is UP, administrative state is UP
      Hardware is Tunnel
      IPv6 address 2001:db8:10:10::1/64
      IPv6 address fe80::21a:ebff:fe92:a4bc/64
      index xxx metric 1 mtu 1476
      <UP,POINTOPOINT,RUNNING,MULTICAST>
      SNMP link-status traps: Disabled
      Tunnel source 10.1.1.1, destination 10.1.1.2
      Tunnel name local 10.1.1.1, remote 10.1.1.2
      Tunnel ID local (not set), remote (not set)
      Tunnel protocol/transport gre, key disabled, sequencing disabled
      Tunnel TTL 64
      Checksumming of packets disabled, path MTU discovery disabled
        input packets 0, bytes 0, dropped 0, multicast packets 0
        output packets 8, bytes 480, multicast packets 0 broadcast packets 0
        input average rate : 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        output average rate: 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        input peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
        output peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
      Time since last state change: 0 days 00:01:29

IPv4 over IPv6トンネルインターフェースtunnel1の情報を表示する。

    awplus> show interface tunnel1
    Interface tunnel1
      Link is UP, administrative state is UP
      Hardware is Tunnel
      IPv4 address 172.16.10.1/24 pointopoint 172.16.10.255
      index xxx metric 1 mtu 1460
      <UP,POINTOPOINT,RUNNING,MULTICAST>
      SNMP link-status traps: Disabled
      Tunnel source 2001:db8:1:1::1, destination 2001:db8:1:1::2
      Tunnel name local 2001:db8:1:1::1, remote 2001:db8:1:1::2
      Tunnel ID local (not set), remote (not set)
      Tunnel protocol/transport ipv6, key disabled, sequencing disabled
      Tunnel TTL 64
      Checksumming of packets disabled, path MTU discovery disabled
        input packets 0, bytes 0, dropped 0, multicast packets 0
        output packets 0, bytes 0, multicast packets 0 broadcast packets 0
        input average rate : 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        output average rate: 30 seconds X.XX Kbps, 5 minutes X.XX Kbps
        input peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
        output peak rate XX.XX Kbps at XXXX/XX/XX XX:XX:XX
      Time since last state change: 0 days 00:17:23

表 1：詳細表示（briefオプション未指定時）
Interface | インターフェース名
Link is | リンクステータス
administrative state is | 管理ステータス。UP（ポートが有効に設定されている）、DOWN（ポートが無効に設定されている）、err-disabled（製品の機能によりポートがブロックされてリンクダウンしている）
Thrash-limiting | 未サポート
Hardware is | インターフェース種別。Ethernet、Loopback、Tunnelなどがある
address is | 物理（MAC）アドレス
DHCP client enabled on interface | 該当インターフェースでDHCPクライアント機能が有効な場合に表示される
IPv4 address | IPアドレス/マスク長。IPアドレスが設定されているときだけ表示される
broadcast | IPブロードキャストアドレス。IPアドレスが設定されているときだけ表示される
IPv6 address | IPv6アドレス/プレフィックス長。IPv6アドレスが設定されているときだけ表示される。該当アドレスの状態がpreferred（優先アドレス）以外の場合は、行末にtentative（暫定アドレス）、DAD failed（暫定アドレスの重複を検出）、deprecated（非推奨アドレス）のいずれかの状態が表示される。また、状態のあとにアスタリスク（*）が表示されている場合、該当アドレスが自動設定されたことを示す。IPv6アドレスの状態についてはshow ipv6 interfaceコマンドのページを参照
Description | インターフェースの説明文
index | インターフェースインデックス番号（ifIndex）
current duplex | 実際のデュプレックスモード。物理インターフェース（eth、port）にだけ表示される
current speed | 実際の通信速度。物理インターフェース（eth、port）にだけ表示される
polarity | 極性。物理インターフェース（eth、port）にだけ表示される
configured duplex | デュプレックスモードの設定値。物理インターフェース（eth、port）にだけ表示される
configured speed | 通信速度の設定値。物理インターフェース（eth、port）にだけ表示される
metric | メトリック
mtu | MTU（Maximum Transmission Unit）
mru | MRU（Maximum Receive Unit）
arp ageing timeout | ARPタイムアウト（ARPエントリー保持時間）
<UP,BROADCAST,RUNNING,MULTICAST> | インターフェースフラグの状態
SNMP link-status traps | SNMPのリンクステータス通知メッセージを生成するかどうか。Sending（生成する）、Disabled（生成しない）のいずれか。Sendingに設定されており、なおかつ、単位時間あたりの生成数に上限が設定されている場合は「(suppressed after 20 traps in 30 sec)」のような形式で上限値も表示される。上限が設定されていない場合は「(suppression disabled)」と表示される
input packets | 受信パケット数。以下、受信パケットに関して、bytes（バイト数）、dropped（破棄パケット数）、multicast packets（マルチキャストパケット数）が表示される
output packets | 送信パケット数。以下、送信パケットに関して、bytes（バイト数）、multicast packets（マルチキャストパケット数）、broadcast packets（ブロードキャストパケット数）が表示される
Time since last state change | 前回ステータス変更後の経過時間

表 2：簡潔表示（briefオプション指定時）
Interface | インターフェース名
Status | 管理ステータス
Protocol | リンクステータス

## 注意・補足事項

各インターフェースのインターフェースインデックス番号（ifIndex）は次のとおり。

表 1
インターフェース種別 | インターフェースインデックス番号（ifIndex）
ループバックインターフェース（lo） | 1
PPPインターフェース（pppX） | 利用可能な番号が内部で自動的に割り当てられる。 ただし、トンネルインターフェースについては、トンネル種別に応じた必要最低限の設定をしないとifIndexは割り当てられない
VAPインターフェース（vapX.Y）
Ethernetインターフェース（ethX）
ブリッジインターフェース（brX）
トンネルインターフェース（tunnelX）
802.1Qサブインターフェース（ethX.Y、tunnelX.Y、br0.Y）

Note

以下のインターフェースは、起動時にインターフェースインデックス番号を採番するため、作成時と異なる場合があります。

- PPPインターフェース（pppX）
- VAPインターフェース（vapX.Y）
- Ethernetインターフェース（ethX）
- ブリッジインターフェース（brX）
- トンネルインターフェース（tunnelX）
- 802.1Qサブインターフェース（ethX.Y、tunnelX.Y、br0.Y）

トンネルインターフェース（tunnelX）と802.1Qトンネルサブインターフェース（tunnelX.Y）、PPPインターフェース（pppX）については、インターフェースダウン/アップ後にもインターフェースインデックス番号を採番するため、インターフェースダウン/アップ後にインターフェースインデックス番号が変わります。
droppedカウンターはカウントされません。
administrative stateのerr-disabledは、製品の機能によってポートがリンクダウンしている場合にのみ表示されます。このため、STPなどの機能によって、リンクアップしたままポートがブロックされている状態となった場合、err-disabledとは表示されずUPと表示されます。

## 関連コマンド