# show cellular

モード
  特権EXECモード
カテゴリー
  インターフェース / USB型データ通信端末

## 構文

コマンド構文

`# show cellular [IFNAME]`

## コマンド説明

USB型データ通信端末の情報を表示する。
Note

データ通信端末の情報はPPP接続を行っていないときにだけ表示可能です。PPP接続中の端末情報は表示されません。

Note

Network Mode（使用回線種別の設定）は直近のPPP接続時にUSB型データ通信端末に設定されていた内容を示します。network-modeコマンドの設定内容とは必ずしも一致しません。

## パラメーター

`IFNAME`
  USB型データ通信端末のインターフェース名（cellularX）

## 使用例

    awplus# show cellular
    Interface cellular0
      Manufacturer: Fujisoft.inc
      Model ID: FS020U
      Revision ID: LQTJC05.1.4_M012
      Serial ID: 123456789012345
      IMSI: 987654321098765
      Active Service Class: Data mode
      Phone Activity Status: Call in progress
      Service Center Address:
        Phone Number: +811234567890
        Number Type: International
      GPRS Mobile Station Class: Class A
      Serial Port Configuration:
        Baud rate: 115200
        Character Format: 8-N-1
        Parity: Space
      Terminal Equipment Character Set: IRA
      Cable interface DTE-DCE local flow control:
        To DTE: RTS
        To DCE: CTS
      System Time: 16/08/24,00:43:22
      GPRS Network Registration Status: Registered, home network
      PIN Request Status: READY
      Functionality Level: Full functionality (power-saving disabled)
      Facility Lock Status:
        SIM card lock: Not active
        SIM fixed dialling memory feature: Not active
        Network personalization: Not active
        Network subset personalization: Not active
        Service provider personalization: Not active
        Corporate personalization: Not active
        Lock phone to first SIM card: Not active
      Call Mode: Single mode
      Wireless Data Service: 3GPP systems (GERAN, UTRAN and E-UTRAN)
      Network Mode: 4G Only
      GPRS Service Status: Mobile station is attached to a GPRS service
      Dialling Number Type: National
      Bearer Service Type:
        Autobauding: Enabled
        Service: Data circuit asynchronous (UDI or 3.1 kHz modem)
        Connection Element: Non-transparent
      Automatic time and time zone update via NITS: Not enabled
      PPP support between TE and MT: Supported
      Last Error Report: No cause information available
      PLMN selection method: User controlled PLMN selected from Access Technology
      PDP Contexts:
        Context ID: 15
          Type: IP
          APN: testname.alliedtelesis
          Address: 0.0.0.0
          Data Compression: Off
          Header Compression: Off
          Status: Not active
        Context ID: 1
          Type: IP
          APN: testname.alliedtelesis
          Address: 0.0.0.0
          Data Compression: Off
          Header Compression: Off
          Status: Active
      Primary DNS: 0.0.0.0
      Secondary DNS: 0.0.0.0
      Diagnostic mode baud rate: 115200
      TE-DCE baud rate: 115200
      Tolerance to long delays in PDP call setup: Enabled
      System Info:
        System Service State: Valid service
        System Service Domain: Only PS service
        Roaming Status: Not roaming
        SIM card state: Valid USIM card state
      System Config:
        Supported System Mode: Auto-select
        Network Acquisition Order: WCDMA, then GSM
        Roaming Support: Supported

## 関連コマンド