# show auth

モード
  特権EXECモード
カテゴリー
  インターフェース / ポート認証

## 構文

コマンド構文

`# show auth [interface [IFRANGE]|all]`

## コマンド説明

ポート認証の全般的情報、および、スイッチポートごとの情報を表示する。
オプションを指定せずに実行した場合は、全般的情報だけが表示される。
interfaceパラメーターを指定した場合は、インターフェースごとの情報だけが表示される。
allオプションを指定した場合は、全般的設定とすべてのインターフェースの情報が表示される。

## パラメーター

`interface [IFRANGE]`
  スイッチポートごとの情報を表示する。特定ポートの情報だけを表示させたいときは、IFRANGEにスイッチポートのインターフェース名を指定する。ハイフン、カンマを使った複数指定も可能。省略時はポート認証の設定が行われているすべてのインターフェースが対象になる
`all`
  システム全体の情報に加え、スイッチポートごとの情報も表示させたいときに指定する

## 使用例

    awplus# show auth interface
    Authentication Info for interface port1.0.1
      portEnabled: false - portControl: Auto
      portStatus: Unknown
      reAuthenticate: disabled
      reAuthPeriod: 3600
      PAE: quietPeriod: 60 - maxReauthReq: 2 - txPeriod: 30
      PAE: connectTimeout: 30
      BE: suppTimeout: 30 - serverTimeout: 30 - maxReq: 2
      CD: adminControlledDirections: in
      KT: keyTxEnabled: false
      critical: disabled
      guestVlan: disabled
      guestVlanForwarding:
        none
      authFailVlan: disabled
      dynamicVlanCreation: disabled
      multiVlanSession: disabled
      hostMode: single-host
      dot1x: disabled
      authMac: enabled
        method: PAP
        reauthRelearning: disabled
      authWeb: disabled
      twoStepAuthentication:
        configured: disabled
        actual: disabled
      supplicantMac: none
      supplicantIpv4: none

## 関連コマンド