# show wireless network

モード
  非特権EXECモード
カテゴリー
  無線LANコントローラー（AWC対応） / 無線ネットワーク設定

## 構文

コマンド構文

`> show wireless network [<1-65535>|all] [brief]`

## コマンド説明

無線ネットワークの設定内容を表示する。

## パラメーター

`<1-65535>`
  無線ネットワーク設定番号。カンマ、ハイフン区切りで複数指定が可能。本パラメーター指定時は指定したネットワークだけを表示する。省略時はallを指定したのと同じ動作となる
`all`
  すべてのネットワークを表示する（省略時動作）
`brief`
  無線ネットワークの情報を簡潔に表示させたいときに指定する。省略時は詳細な情報が表示される

## 使用例

    awplus> show wireless network
    Network ID 1:
     Description ...................
     Assigned VLAN ID .............. 1
     SSID .......................... web-click
     Hide SSID ..................... -
     Emergency Mode ................ Disable
     Band-Steering ................. Disable
     Association Advertisement ..... Disable
     Duplicate AUTH Received ....... Disconnect
     DTIM Period ................... 1
     Proxy ARP ..................... Disable
      ARP Pass Through ............. Disable
     BSS Transition Management ..... Disable
     Security ID ................... -
      Security Mode ................ -
     MAC-Auth
      Authentication Mode .......... none
      RADIUS group .................
      Username
       Separator ................... hyphen
       Character Case .............. lower-case
      Password .....................
      RADIUS Send Service Type ..... Disable
      RADIUS DAC IP Address ........
      RADIUS Calling-Station-Id
       Separator ................... hyphen
       Character Case .............. upper-case
      Verify RADIUS Packets ........ Disable
      Dynamic VLAN ................. Disable
      Critical Mode ................ Disable
     RADIUS group for Web-Auth .....
     Two-step authentication ....... Enable
     Wireless MAC filter ID ........
     Wireless Trigger ID ........... 0
     Inactivity Timer .............. 300
     Client Isolation Mode ......... Disabled
     Unassociated Client List ...... Not acquire
     Airtime Percentage ............ 0
     Multicast Unicast conversion .. Disable
     Disconnect Low-Signal Clients . Disable
     RSSI Threshold ................ -75
     Captive-Portal ................ Enable
      Authentication Mode .......... click-through
      Auth Page Language ........... Japanese
      Agreement Message Text
       ID  1:
        Language ................... en
        Textfile ................... clicken.txt
       ID  2:
        Language ................... ja
        Textfile ................... clickja.txt
      RADIUS group .................
      RADIUS Accounting  ........... Disable
      External Page URL ............
      Redirect URL .................
      Session keep ................. Disable
      Session Timeout Interval ..... 3600
      Session Timeout Action . ..... Reauthentication
      Page proxy URL ...............
      Walled Garden Entries ........ 0
      DNS Proxy for Walled Garden .. Disable
      Verify RADIUS Packets ........ Disable
     Passpoint ..................... Disable
     :
     :

    awplus> show wireless network brief
    ID    VLAN SSID                             H E Sec ID MAC-Auth Web-Auth
    ----- ---- -------------------------------- - - ------ -------- --------
        1    1 web-click                        - -      -        -        -
    65533    1 Management                       - -  65533        -        -
    65534    1 Engineer                         - -  65534        -        -
    65535    1 Sales                            - -  65535        -        -

## 関連コマンド