# show application detail

モード
  特権EXECモード
カテゴリー
  UTM / アプリケーション定義

## 構文

コマンド構文

`# show application detail [NAME|custom|dpi]`

## コマンド説明

アプリケーション定義の詳細情報（定義名、プロトコル、その他詳細）を表示する。
オプションパラメーターを省略した場合はすべてのアプリケーション定義が対象となる。

## パラメーター

`NAME`
  アプリケーション定義名。指定したアプリケーション定義だけを表示する
`custom`
  ユーザーがapplicationコマンドで作成したカスタムアプリケーション定義だけを表示する
`dpi`
  アプリケーションコントロール（DPI = ディープパケットインスペクション）機能によって判別可能なアプリケーションの一覧を表示する。表示内容は現在使用しているアプリケーションシグネチャデータベース（providerコマンド）によって異なる

## 使用例

アプリケーション定義の内容を一覧表示する。

    awplus# show application detail
    Name             Protocol    Detail
    --------------------------------------------------------------------------
    aim              TCP         sport=1024-65535 dport=9898
    cvs              TCP         sport=1024-65535 dport=2401
    dns              UDP         sport=1024-65535 dport=53
    esp              50          -
    ftp              TCP         sport=1024-65535 dport=21
    http             TCP         sport=1024-65535 dport=80
    https            TCP         sport=1024-65535 dport=443
    icq              TCP         sport=1024-65535 dport=5190
    ident            TCP         sport=1024-65535 dport=113
    imap             TCP         sport=1024-65535 dport=143
    imaps            TCP         sport=1024-65535 dport=993
    irc              TCP         sport=1024-65535 dport=6667
    isakmp           UDP         sport=500 dport=500
    jabber           TCP         sport=1024-65535 dport=5222-5223
    l2tp             UDP         sport=1701 dport=1701
    ldap             TCP         sport=1024-65535 dport=389
    lisa             TCP         sport=1024-65535 dport=7741
    msn              TCP         sport=1024-65535 dport=1863
    mydb             TCP         sport=1024-65535 dport=8704
    mysql            TCP         sport=1024-65535 dport=3306
    mystream         UDP         sport=1024-65535 dport=50000-50099,51024
    news             TCP         sport=1024-65535 dport=119
    nfs-tcp          TCP         sport=1024-65535 dport=2049
    nfs-udp          UDP         sport=1024-65535 dport=2049
    ntp              UDP         sport=123,1024-65535 dport=123
    openvpn          UDP         sport=1024-65535 dport=1194
    path-mtu-ipv4    ICMP        type=3 code=4
    path-mtu-ipv6    IPv6-ICMP   type=2 code=0
    pcanywhere-tcp   TCP         sport=1024-65535 dport=5631
    pcanywhere-udp   UDP         sport=1024-65535 dport=5631-5632
    ping             ICMP        type=8 code=0
    pop3             TCP         sport=1024-65535 dport=110
    pop3s            TCP         sport=1024-65535 dport=995
    pptp             TCP         sport=1024-65535 dport=1723
    rdp              TCP         sport=1024-65535 dport=3389
    rsync            TCP         sport=1024-65535 dport=873
    samba-tcp        TCP         sport=1024-65535 dport=139,445
    samba-udp        UDP         sport=137-138,1024-65535 dport=137-138
    smtp             TCP         sport=1024-65535 dport=25
    socks            TCP         sport=1024-65535 dport=1080
    ssh              TCP         sport=1024-65535 dport=22
    syslog           UDP         sport=1024-65535 dport=514
    telnet           TCP         sport=1024-65535 dport=23
    traceroute       UDP         sport=1024-65535 dport=33434-33523
    vnc              TCP         sport=1024-65535 dport=5900
    whois            TCP         sport=1024-65535 dport=43

ユーザーが作成したカスタムアプリケーション定義の内容だけを表示する。

    awplus# show application detail custom
    Name             Protocol    Detail
    --------------------------------------------------------------------------
    esp              50          -
    isakmp           UDP         sport=500 dport=500
    mydb             TCP         sport=1024-65535 dport=8704
    mystream         UDP         sport=1024-65535 dport=50000-50099,51024
    path-mtu-ipv4    ICMP        type=3 code=4
    path-mtu-ipv6    IPv6-ICMP   type=2 code=0

DPIアプリケーションの一覧を表示する。
製品内蔵データベース（built-in）を使用している場合

    awplus# show application detail dpi
    Name              Mark    Detail
    --------------------------------------------------------------------------------
    afp               0x6A    DPI: Apple Filing Protocol, formerly AppleTalk
                                (Cat=File transfer)
    aimini            0x6C    DPI: Aimini P2P real-time communicatings
                                (Cat=Messaging)
    ajp               0x94    DPI: Apache JServ Protocol (Cat=Networking)
    amazon            0xBB    DPI: Amazon online shopping (Cat=Web Services)
    amazonvideo       0xF9    DPI: Amazon on-demand video streaming service
                                (Cat=Streaming Media)
    amqp              0xC9    DPI: Advanced Message Queuing Protocol
                                (Cat=Networking)
    apple             0x95    DPI: Apple Inc website (Cat=Networking)
    appleicloud       0x98    DPI: A cloud storage and cloud computing service from
                                Apple Inc (Cat=File transfer)
    appleitunes       0x9A    DPI: A media streaming, broadcasting, and device
                                management application from Apple Inc
                                (Cat=Streaming Media)
    applejuice        0x21    DPI: A defunct file sharing protocol (Cat=File
                                transfer)
    applepush         0xF7    DPI: Apple Push Notification Service (Cat=Social
                                Networking)
    applestore        0xE9    DPI: Online store for applications that run on
                                Apple's operating systems (Cat=File transfer)
    appletalk         0x7     DPI: A proprietary suite of networking protocols
                                developed by Apple Inc
    armagetron        0x71    DPI: Armagetron multiplayer online game (Cat=Games)
    arp               0x4     DPI: Address Resolution Protocol
    atmf              0x9     DPI: Allied Telesis Management Framework
    ...

サンドバイン社のデータベース（procera）を使用している場合

    awplus# show application detail dpi
    Name              Mark    Detail
    --------------------------------------------------------------------------------
    050plus           0x435   DPI: The traffic consists of data from logging in or
                                making calls with the 050Plus application.
                                (Cat=Messaging, Prod=2, Risk=2)
    12306cn           0x292   DPI: 12306.cn is the only China Railway customer
                                service center (Cat=Web Services, Prod=4, Risk=1)
    123movie          0x64D   DPI: Free movie streaming/downloading site
                                (Cat=Streaming Media, Prod=1, Risk=5)
    126com            0x293   DPI: 126.com is a free webmail service of Netease
                                (Cat=Mail, Prod=4, Risk=2)
    17173             0x30B   DPI: General browsing, interaction, and game play on
                                the social gaming network 17173.com (Cat=Social
                                Networking, Prod=2, Risk=2)
    1fichier          0x779   DPI: Online cloud storage. (Cat=File Transfer, Prod=1,
                                Risk=5)
    2345com           0x2BE   DPI: General browsing of navigation portal 2345.com
                                (Cat=Web Services, Prod=3, Risk=1)
    247inc            0x36D   DPI: Data and advertisements hosted by [24]7 Inc.
                                (Cat=Web Services, Prod=3, Risk=1)
    247media          0x36E   DPI: Ads hosted by 24/7 Media technology and the Real
                                Media group. (Cat=Web Services, Prod=3, Risk=1)
    2channel          0x64E   DPI: 2channel is a Japanese textboard (Cat=Social
                                Networking, Prod=1, Risk=3)
    ...

## 関連コマンド